{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["테이블","제품 특징","Sheet1"],"not_rendered":{"charts":0,"images":1,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"테이블","index":0,"n_rows":61,"n_cols":6,"rows_kept":61,"cut":false,"hidden":false,"merged":[]}
[]
[null,"작업용 다목적테이블"]
{"$rows_empty":25}
[null,"   1400×500×720 (W×D×H)          "]
[]
[]
[]
[]
[]
[]
[null,null,"   ·  상     판",null,null,": 23t PB + 양면 LPM + ABS 엣지"]
[]
[null,null,"   ·  다리파이프 ",null,null,": Ø38 원형파이프 (1.4t) + 20X30 각파이프 (1.4t)"]
[null,"자   재"]
[null,null,"   ·  보강파이프 ",null,null,": 20X30 각파이프 (1.4t)"]
[]
[null,null,"   ·  도장 마감",null,null,": 분체도장 "]
{"$rows_empty":8}
[null,null," ·","상     판",":","가재단 → 정재단 → 엣지접착 → 세공"]
[]
[null,"제작공정"," ·","다리파이프",":","절단/노칭 → 용접 → 타공 → 분체도장"]
[]
[null,null," ·","보강파이프",":","절단 → 타공 → 용접 → 분체도장"]
[]
[]
[]
[]
[]
[]
[null,"※ 본 시방서의 내용은 계속되는 제품의 연구, 개발로 인해 일부 변경될 수 있습니다."]

{"sheet":"제품 특징","index":1,"n_rows":62,"n_cols":15,"rows_kept":62,"cut":false,"hidden":false,"merged":[]}
[]
[null,"  CRN1 series",{"$nulls":12},"DINING TABLE"]
{"$rows_empty":24}
[null,"테이블 1400*500*720"]
{"$rows_empty":7}
[null,"제품특징","  · 작업 공간에 적합한 다목적 테이블"]
[]
[null,"(기  능)","  · 경량화된 구조로 배치 변경 시 이동이 용이"]
{"$rows_empty":10}
[null,null,"  · 심플한 철재 하부 프레임과 목재 상판으로 간결한 느낌 부여"]
[]
[]
[]
[null,"제품특징"]
[]
[null,"(디자인)"]
{"$rows_empty":7}
[null,"※ 본 시방서의 내용은 계속되는 제품의 연구, 개발로 인해 일부 변경될 수 있습니다."]

{"sheet":"Sheet1","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}