{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["원가계산서_인테리어","총괄 집계표","내역서_인테리어"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":23,"defined_names":121,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"원가계산서_인테리어","index":0,"n_rows":28,"n_cols":7,"rows_kept":28,"cut":false,"hidden":false,"merged":[[27,1,27,3],[21,1,21,3],[22,1,22,3],[23,1,23,3],[24,1,24,3],[25,1,25,3],[26,1,26,3],[0,1,0,6],[1,1,1,4],[1,5,1,6],[2,1,2,3],[3,1,20,1],[3,2,6,2],[7,2,9,2],[10,2,20,2]],"flags":["formulas_cached_only"]}
[null," 공 사 원 가 계 산 서"]
[null,"공사명 : 부천대학교 소사캠퍼스 3F 치기공과 신설공사"]
[null,"비        목",null,null,"금      액","구        성        비","비      고"]
["A1","순   공   사   원   가","재   료   비","직  접  재  료  비",0,"자재비",""]
["A2",null,null,"간  접  재  료  비",null,"",""]
["A3",null,null,"작업설, 부산물(△)",null,"",""]
["AS",null,null,"[ 소          계 ]",0,"",""]
["B1",null,"노   무   비","직  접  노  무  비",0,"인건비(노무비)",""]
["B2",null,null,"간  접  노  무  비",0,"직접노무비 * 2.0%"]
["BS",null,null,"[ 소          계 ]",0,""]
["C4",null,"경비","산  재  보  험  료",0,"노무비 * 3.7%"]
["C5",null,null,"고  용  보  험  료",0,"노무비 *1.01%"]
["C6",null,null,"국민  건강  보험료",0,"직접노무비 * 3.43%"]
["C7",null,null,"국민  연금  보험료",0,"직접노무비 * 4.5%"]
["C9",null,null,"노인장기요양보험료",0,"국민건강보험료 * 11.52%"]
["CA",null,null,"산업안전보건관리비",0,"(재료비+직노) * 2.93%"]
["CG",null,null,"기   타    경   비",0,"(재료비+노무비) * 1.5%"]
["CG",null,null,"환경보전비",0,"직접공사비*0.3%"]
["CG",null,null,"퇴직공제부금비",0,"직접노무비*2.3%"]
["CG",null,null,"공사이행보증수수료",null,"직접공사비*0.0355%*공기(년)"]
["CS",null,null,"[ 소          계 ]",0,""]
["S1","        계",null,null,0,""]
["D1","일  반  관  리  비",null,null,0,"계 * 3%"]
["D2","이              윤",null,null,0,"(노무비+경비+일반관리비) * 7.0%"]
["D9","공   급    가   액",null,null,0,"",""]
["DB","부  가  가  치  세",null,null,0,"공급가액 * 10%",""]
["DH","도      급      액",null,null,0,"",""]
["S2","총   공   사    비",null,null,0,"",""]

{"sheet":"총괄 집계표","index":1,"n_rows":37,"n_cols":14,"rows_kept":37,"cut":false,"hidden":false,"merged":[[2,10,2,11],[2,12,3,12],[2,13,3,13],[2,0,3,0],[2,1,3,1],[2,2,3,2],[2,3,3,3],[2,4,3,4],[2,5,3,5],[2,6,3,6],[2,7,3,7],[2,8,2,9]],"flags":["formulas_cached_only"]}
["2021  INTERIOR STANDARD ESTIMATE"]
[null,"집계표"]
["번호","명       칭","제조사","모델 No.","규  격","단위","수  량","자재\nloss율","자 재 비",null,"인 건 비",null,"합 계","비  고"]
[{"$nulls":8},"단  가","금액","단  가","금액"]
[]
["■","총괄 집계표"]
[null,"직접 공사비"]
[]
["A","인테리어 공사",null,null,null,"LOT",1,null,null,0,null,0,0]
{"$rows_empty":27}
[null,"직접공사비 계",{"$nulls":7},0,null,0,0]

{"sheet":"내역서_인테리어","index":2,"n_rows":419,"n_cols":14,"rows_kept":419,"cut":false,"hidden":false,"merged":[[2,9,2,10],[2,12,3,12],[2,0,3,0],[2,1,3,1],[2,2,3,2],[2,3,3,3],[2,11,3,11],[2,4,3,4],[401,2,401,3],[387,2,387,4],[4,0,4,2],[2,5,3,5],[2,6,3,6],[2,7,2,8]],"flags":["formulas_cached_only"]}
["2021  INTERIOR STANDARD ESTIMATE"]
["내역서"]
["번호","명       칭","모델 No.","규  격","단위","수량","자재\nloss율","자 재 비",null,"인 건 비",null,"합 계","비  고"]
[{"$nulls":7},"단  가","금액","단  가","금액"]
["부천대 소사캠퍼스 3F 치기공과 신설공사"]
[]
["A","인테리어 공사"]
["1","가설 및 기타 공사",{"$nulls":6},0,null,0,0]
["2","철거공사",{"$nulls":6},0,null,0,0]
["3","치과재료학 실습실",{"$nulls":6},0,null,0,0]
["4","기초기공 실습실",{"$nulls":6},0,null,0,0]
["5","고정성보철기공 실습실",{"$nulls":6},0,null,0,0]
["6","치과모형 작업실",{"$nulls":6},0,null,0,0]
["7","복도공사",{"$nulls":6},0,null,0,0]
["8","남.여 탈의실공사",{"$nulls":6},0,null,0,0]
["9","설비공사",{"$nulls":6},0,null,0,0]
["10","공조 및 냉.난방 공사",{"$nulls":6},0,null,0,0]
{"$rows_empty":28}
[null,"인테리어공사비 계",{"$nulls":6},0,null,0,0]
["1","가설 및 기타 공사"]
[null,"먹메김",null,null,"M2",360.9,1,null,0,null,0,0]
[null,"내부 수평 비계",null,null,"M2",360.9,1,null,0,null,0,0]
[null,"현장정리",null,null,"M2",360.9,1,null,0,null,0,0]
[null,"현장 보양",null,null,"M2",360.9,1,null,0,null,0,0]
[null,"자재양중",null,"대.소운반","인",30,1,null,0,null,0,0]
[null,"준공청소",null,null,"M2",360.9,1,null,0,null,0,0]
[null,"실리콘 마감",null,null,"식",1,1,null,0,null,0,0]
[null,"운임비",null,"목자재 외","대",6,1,null,0,null,0,0]
[null,"폐자재 처리 차량","공사 중","1.5TON","대",6,1,null,0,null,0,0]
[null,"가설설치(도어 포함)",null,"샌드위치판넬","M2",6.48,1,null,0,null,0,0]
[null,"가설철거",null,"폐기물 포함","식",1,1,null,0,null,0,0]
[null,"조명제어 프로그램 세팅",null,null,"식",1,1,null,0,null,0,0]
[]
[null,"합       계",{"$nulls":6},0,null,0,0]
[]
["2","철거공사"]
[null,"석면검사비",null,"석면함유/특정폐기물","식",1,1,null,0,null,0,0]
[null,"바닥_P-TILE철거",null,null,"M2",394.90000000000003,1,null,0,null,0,0]
[null,"천정 철거",null,null,"M2",394.90000000000003,1,null,0,null,0,0]
[null,"벽체 철거_경량",null,null,"M2",227.92000000000002,1,null,0,null,0,0]
[null,"집기류 철거",null,null,"식",1,1,null,0,null,0,0]
[null,"소운반",null,null,"인",12,1,null,0,null,0,0]
[null,"폐기물",null,"2.5TON","대",6,1,null,0,null,0,0]
[]
[null,"합       계",{"$nulls":6},0,null,0,0]
[]
["3","치과재료학 실습실"]
[null,"<벽체 공사>"]
[null,"벽체 구조틀",null,null,"M2",102.48,1.1,null,0,null,0,0]
[null,"스카이비바_흡음 단열재",null,"24k 50T","M2",35.15,1.1,null,0,null,0,0]
[null,"합판보강",null,"9T 합판 1ply","M2",88.98,1.1,null,0,null,0,0]
[null,"석고보드",null,"석고보드 9.5T 1ply","M2",83.16,1.1,null,0,null,0,0]
[null,"라인 흡음보드",null,"1200*2400*9T","M2",27,1.15,null,0,null,0,0]
[null,"후면 키큰장 제작",null,null,"식",1,1,null,0,null,0,0]
[null,"후면 게이트 몰딩",null,"MDF 30T","M",26,1.1,null,0,null,0,0]
[null,"템바보드",null,null,"M2",5.4,1.15,null,0,null,0,0]
[null,"모니터 베이스 구조틀",null,"ㅁ40*40","M2",22.14,1.15,null,0,null,0,0]
[null,"백페인트 테두리 조성",null,"SUS H/L 10*20","M",29.72,1.15,null,0,null,0,0]
[null,"필경대",null,"SUS H/L 매입형","M",3.2,1.15,null,0,null,0,0]
[null,"백페인트 글라스",null,"지정칼라","자평",150,1,null,0,null,0,0]
[null,"걸레받이 취부",null,"SUS H/L 10*100","M",32.7,1.1,null,0,null,0,0]
[null,"벽체 PUTTY",null,"줄퍼티 2회, 올퍼티 1회","M2",115.56,1,null,0,null,0,0]
[null,"벽체 수성도장",null,"지정칼라","M2",115.56,1,null,0,null,0,0]
[null,"후면 싱크장 벽체 타일 취부","75*300","백색 무광지정타일","M2",13.799999999999999,1.1,null,0,null,0,0]
[null,"타일 부자재",null,"세라픽스","M2",13.799999999999999,1.1,null,0,null,0,0]
[null,"강의실 사인물",null,null,"식",1,1,null,0,null,0,0]
[]
[null,"<천정 공사>"]
[null,"천정 구조틀",null,"T-BAR","M2",57.1,1.1,null,0,null,0,0]
[null,"마이톤",null,"600*600","M2",57.1,1.1,null,0,null,0,0]
[null,"천정 구조틀",null,"LGS M-BAR","M2",32.7,1.1,null,0,null,0,0]
[null,"석고보드(테두리 마감 포함)",null,"석고보드 9.5T 2ply","M2",32.7,1.1,null,0,null,0,0]
[null,"천정 몰딩",null,"갈바 1.2T 15*25","M",31.9,1.1,null,0,null,0,0]
[null,"커튼박스",null,"갈바 1.2T 절곡","M",6.239999999999999,1.1,null,0,null,0,0]
[null,"블라인드",null,"선스크린","M2",16.848,1.1,null,0,null,0,0]
[null,"천정 PUTTY",null,"줄퍼티 2회, 올퍼티 1회","M2",32.7,1,null,0,null,0,0]
[null,"천정 수성도장",null,"지정칼라","M2",32.7,1,null,0,null,0,0]
[null,"유성도장",null,"지정칼라","M",38.14,1,null,0,null,0,0]
[]
[null,"<바닥 공사>"]
[null,"셀프레벨링",null,null,"M2",94.1,1.05,null,0,null,0,0]
[null,"PTILE",null,"LG 600*600 ","M2",94.1,1.05,null,0,null,0,0]
[null,"부자재",null,null,"M2",94.1,1,null,0,null,0,0]
[]
[null,"<조명 공사>"]
[null,"사각 평판등",null,"600*600","EA",18,1,null,0,null,0,0]
[null,"6인치 매입등",null,"6인치","EA",24,1,null,0,null,0,0]
[null,"T-5",null,"LED L:1200","EA",5,1,null,0,null,0,0]
[null,"LED_BAR",null,null,"M",20.556,1,null,0,null,0,0]
[null,"SMPS",null,"12V 100W","EA",2,1,null,0,null,0,0]
[null,null,null,"12V 150W","EA",3,1,null,0,null,0,0]
[]
[null,"<가구 공사>"]
[null,"진열장",null,"지정도장마감","자",23.5,1,null,0,null,0,0]
[null,"상부 수납장",null,"지정도장마감","자",20,1,null,0,null,0,0]
[]
[null,"합       계",{"$nulls":6},0,null,0,0]
[]
["4","기초기공 실습실"]
[null,"<벽체 공사>"]
[null,"벽체 구조틀",null,null,"M2",122.79000000000002,1.1,null,0,null,0,0]
[null,"스카이비바_흡음 단열재",null,"24k 50T","M2",31.080000000000002,1.1,null,0,null,0,0]
[null,"합판보강",null,"9T 합판 1ply","M2",122.79000000000002,1.1,null,0,null,0,0]
[null,"석고보드",null,"석고보드 9.5T 1ply","M2",55.620000000000005,1.1,null,0,null,0,0]
[null,"라인 흡음보드",null,"1200*2400*9T","M2",27.27,1.15,null,0,null,0,0]
[null,"후면 키큰장 제작",null,null,"식",1,1,null,0,null,0,0]
[null,"후면 게이트 몰딩",null,"MDF 30T","M",25.2,1.1,null,0,null,0,0]
[null,"템바보드",null,null,"M2",4.6,1.15,null,0,null,0,0]
[null,"모니터 베이스 구조틀",null,"ㅁ40*40","M2",22.14,1.15,null,0,null,0,0]
[null,"백페인트 테두리 조성",null,"SUS H/L 10*20","M",18.400000000000002,1.15,null,0,null,0,0]
[null,"필경대",null,"SUS H/L 매입형","M",3.2,1.15,null,0,null,0,0]
[null,"백페인트 글라스",null,"지정칼라","자평",136,1,null,0,null,0,0]
[null,"걸레받이 취부",null,"SUS H/L 10*100","M",32.7,1.1,null,0,null,0,0]
[null,"벽체 PUTTY",null,"줄퍼티 2회, 올퍼티 1회","M2",87.49,1,null,0,null,0,0]
[null,"벽체 수성도장",null,"지정칼라","M2",87.49,1,null,0,null,0,0]
[null,"후면 싱크장 벽체 타일 취부","75*300","백색 무광지정타일","M2",13.799999999999999,1.1,null,0,null,0,0]
[null,"타일 부자재",null,"세라픽스","M2",13.799999999999999,1.1,null,0,null,0,0]
[null,"강의실 사인물",null,null,"식",1,1,null,0,null,0,0]
[]
[null,"<천정 공사>"]
[null,"천정 구조틀",null,"T-BAR","M2",57.1,1.1,null,0,null,0,0]
[null,"마이톤",null,"600*600","M2",57.1,1.1,null,0,null,0,0]
[null,"천정 구조틀",null,"LGS M-BAR","M2",34.2,1.1,null,0,null,0,0]
[null,"석고보드(테두리 마감 포함)",null,"석고보드 9.5T 2ply","M2",34.2,1.1,null,0,null,0,0]
[null,"천정 몰딩",null,"갈바 1.2T 15*25","M",31.9,1.1,null,0,null,0,0]
[null,"커튼박스",null,"갈바 1.2T 절곡","M",6.2,1.1,null,0,null,0,0]
[null,"블라인드",null,"선스크린","M2",16.740000000000002,1.1,null,0,null,0,0]
[null,"천정 PUTTY",null,"줄퍼티 2회, 올퍼티 1회","M2",34.2,1,null,0,null,0,0]
[null,"천정 수성도장",null,"지정칼라","M2",34.2,1,null,0,null,0,0]
[null,"유성도장",null,"지정칼라","M",38.1,1,null,0,null,0,0]
[]
[null,"<바닥 공사>"]
[null,"악세스플로어",null,"STEEL / 600*600 전도성타일","M2",95,1.05,null,0,null,0,0]
[null,"플로어 타공",null,"배관 인입부","개소",37,1,null,0,null,0,0]
[null,"부자재",null,null,"M2",95,1,null,0,null,0,0]
[]
[null,"<조명 공사>"]
[null,"사각 평판등",null,"600*600","EA",18,1,null,0,null,0,0]
[null,"6인치 매입등",null,"6인치","EA",24,1,null,0,null,0,0]
[null,"T-5",null,"LED L:1200","EA",5,1,null,0,null,0,0]
[null,"LED_BAR",null,null,"M",13.829999999999998,1,null,0,null,0,0]
[null,"SMPS",null,"12V  60W","EA",2,1,null,0,null,0,0]
[null,null,null,"12V 150W","EA",3,1,null,0,null,0,0]
[]
[null,"<가구 공사>"]
[null,"진열장",null,"지정도장마감","자",24,1,null,0,null,0,0]
[null,"상부 수납장",null,"지정도장마감","자",20,1,null,0,null,0,0]
[]
[null,"합       계",{"$nulls":6},0,null,0,0]
[]
["5","고정성보철기공 실습실"]
[null,"<벽체 공사>"]
[null,"벽체 구조틀",null,null,"M2",137.59,1.1,null,0,null,0,0]
[null,"스카이비바_흡음 단열재",null,"24k 50T","M2",38.849999999999994,1.1,null,0,null,0,0]
[null,"합판보강",null,"9T 합판 1ply","M2",137.59,1.1,null,0,null,0,0]
[null,"석고보드",null,"석고보드 9.5T 1ply","M2",60.35999999999999,1.1,null,0,null,0,0]
[null,"라인 흡음보드",null,"1200*2400*9T","M2",34.5,1.15,null,0,null,0,0]
[null,"모니터 베이스 구조틀",null,"ㅁ40*40","M2",22.14,1.15,null,0,null,0,0]
[null,"백페인트 테두리 조성",null,"SUS H/L 10*20","M",34.4,1.15,null,0,null,0,0]
[null,"필경대",null,"SUS H/L 매입형","M",4.4,1.15,null,0,null,0,0]
[null,"백페인트 글라스",null,"지정칼라","자평",172,1,null,0,null,0,0]
[null,"유리 프레임 조성",null,"SUS H/L 150*30","M",22.900000000000002,1,null,0,null,0,0]
[null,"도어틀 조성",null,"SUS H/L 180*30","M",5.7,1,null,0,null,0,0]
[null,"가마찌도어 제작_부속품 포함",null,"SUS H/L","SET",1,1,null,0,null,0,0]
[null,"강화유리",null,"10T 면취","자평",127,1,null,0,null,0,0]
[null,"걸레받이 취부",null,"SUS H/L 10*100","M",40.60000000000001,1.1,null,0,null,0,0]
[null,"벽체 PUTTY",null,"줄퍼티 2회, 올퍼티 1회","M2",94.85999999999999,1,null,0,null,0,0]
[null,"벽체 수성도장",null,"지정칼라","M2",94.85999999999999,1,null,0,null,0,0]
[null,"후면 싱크장 벽체 타일 취부","75*300","백색 무광지정타일","M2",11.8,1.1,null,0,null,0,0]
[null,"타일 부자재",null,"세라픽스","M2",11.8,1.1,null,0,null,0,0]
[null,"강의실 사인물",null,null,"식",1,1,null,0,null,0,0]
[]
[null,"<천정 공사>"]
[null,"천정 구조틀",null,"T-BAR","M2",49.2,1.1,null,0,null,0,0]
[null,"마이톤",null,"600*600","M2",49.2,1.1,null,0,null,0,0]
[null,"천정 구조틀",null,"LGS M-BAR","M2",62.3,1.1,null,0,null,0,0]
[null,"석고보드(테두리 마감 포함)",null,"석고보드 9.5T 2ply","M2",62.3,1.1,null,0,null,0,0]
[null,"천정 몰딩",null,"갈바 1.2T 15*25","M",29.6,1.1,null,0,null,0,0]
[null,"라인등 베이스",null,"갈바 1.2T 10*40*10*80","M",48.8,1.1,null,0,null,0,0]
[null,"커튼박스",null,"갈바 1.2T 절곡","M",6.299999999999999,1.1,null,0,null,0,0]
[null,"블라인드",null,"선스크린","M2",17.01,1.1,null,0,null,0,0]
[null,"천정 PUTTY",null,"줄퍼티 2회, 올퍼티 1회","M2",62.3,1,null,0,null,0,0]
[null,"천정 수성도장",null,"지정칼라","M2",62.3,1,null,0,null,0,0]
[null,"유성도장",null,"지정칼라","M",84.7,1,null,0,null,0,0]
[]
[null,"<바닥 공사>"]
[null,"악세스플로어",null,"STEEL / 600*600 전도성타일","M2",115.3,1.05,null,0,null,0,0]
[null,"플로어 타공",null,"배관 인입부","개소",36,1,null,0,null,0,0]
[null,"부자재",null,null,"M2",115.3,1,null,0,null,0,0]
[]
[null,"<조명 공사>"]
[null,"6인치 매입등",null,"6인치","EA",28,1,null,0,null,0,0]
[null,"레일",null,null,"M",38.8,1,null,0,null,0,0]
[null,"레일_전.마",null,null,"EA",4,1,null,0,null,0,0]
[null,"레일_'ㅡ'연결",null,null,"EA",8,1,null,0,null,0,0]
[null,"라인레일등",null,"L:1200","EA",32,1,null,0,null,0,0]
[null,"LED_BAR",null,null,"M",18.509999999999998,1,null,0,null,0,0]
[null,"SMPS",null,"12V  60W","EA",2,1,null,0,null,0,0]
[null,null,null,"12V  100W","EA",2,1,null,0,null,0,0]
[null,null,null,"12V 150W","EA",3,1,null,0,null,0,0]
[]
[null,"<가구 공사>"]
[null,"진열장",null,"지정도장마감","자",29.1,1,null,0,null,0,0]
[null,"키큰장",null,"지정도장마감","SET",2,1,null,0,null,0,0]
[]
[null,"합       계",{"$nulls":6},0,null,0,0]
[]
["6","치과모형 작업실"]
[null,"<벽체 공사>"]
[null,"벽체 구조틀",null,null,"M2",63.27000000000001,1.1,null,0,null,0,0]
[null,"스카이비바_흡음 단열재",null,"24k 50T","M2",37,1.1,null,0,null,0,0]
[null,"합판보강",null,"9T 합판 1ply","M2",91.23,1.1,null,0,null,0,0]
[null,"석고보드",null,"석고보드 9.5T 1ply","M2",76.23,1.1,null,0,null,0,0]
[null,"차음석고보드",null,"석고보드 12.5T 1ply","M2",30,1.1,null,0,null,0,0]
[null,"걸레받이 취부",null,"SUS H/L 10*100","M",35.3,1.1,null,0,null,0,0]
[null,"벽체 PUTTY",null,"줄퍼티 2회, 올퍼티 1회","M2",55.16000000000001,1,null,0,null,0,0]
[null,"벽체 수성도장",null,"지정칼라","M2",55.16000000000001,1,null,0,null,0,0]
[null,"후면 싱크장 벽체 타일 취부","75*300","백색 무광지정타일","M2",34.71,1.1,null,0,null,0,0]
[null,"타일 부자재",null,"세라픽스","M2",34.71,1.1,null,0,null,0,0]
[null,"강의실 사인물",null,null,"식",1,1,null,0,null,0,0]
[]
[null,"<천정 공사>"]
[null,"천정 구조틀",null,"T-BAR","M2",53.5,1.1,null,0,null,0,0]
[null,"마이톤",null,"600*600","M2",53.5,1.1,null,0,null,0,0]
[null,"커튼박스",null,"갈바 1.2T 절곡","M",3.2499999999999996,1.1,null,0,null,0,0]
[null,"블라인드",null,"선스크린","M2",8.91,1.1,null,0,null,0,0]
[null,"유성도장",null,"지정칼라","M",3.2499999999999996,1,null,0,null,0,0]
[]
[null,"<바닥 공사>"]
[null,"악세스플로어",null,"STEEL / 600*600 전도성타일","M2",56.5,1.05,null,0,null,0,0]
[null,"플로어 타공",null,"배관 인입부","개소",15,1,null,0,null,0,0]
[null,"부자재",null,null,"M2",56.5,1,null,0,null,0,0]
[null,"방진매트",null,"방진고무판 300*300*40T","M2",4.3,1.05,null,0,null,0,0]
[]
[null,"<조명 공사>"]
[null,"사각 평판등",null,"600*600","EA",11,1,null,0,null,0,0]
[null,"T-5",null,"LED L:1200","EA",7,1,null,0,null,0,0]
[]
[null,"<가구 공사>"]
[null,"상부 수납장",null,"지정도장마감","자",29.1,1,null,0,null,0,0]
[]
[null,"합       계",{"$nulls":6},0,null,0,0]
[]
["7","복도공사"]
[null,"<천정 공사>"]
[null,"천정 구조틀",null,"CLIP-BAR","M2",55.2,1.1,null,0,null,0,0]
[null,"부자재",null,null,"식",1,1,null,0,null,0,0]
[null,"SMC취부",null,"기존 재사용","M2",55.2,1,null,0,null,0,0]
[]
[null,"<벽체 공사>"]
[null,"기존 벽체 보수 및 도장",null,"지정 칼라","M2",133.92000000000002,1,null,0,null,0,0]
[null,"부자재",null,null,"식",1,1,null,0,null,0,0]
[]
[null,"합       계",{"$nulls":6},0,null,0,0]
[]
["8","남.여 탈의실공사"]
[null,"<벽체 공사>"]
[null,"벽체 구조틀",null,null,"M2",10,1.1,null,0,null,0,0]
[null,"합판보강",null,"9T 합판 1ply","M2",20.4,1.1,null,0,null,0,0]
[null,"석고보드",null,"석고보드 9.5T 1ply","M2",20.4,1.1,null,0,null,0,0]
[null,"걸레받이 취부",null,"MDF 9T","M",10.2,1.1,null,0,null,0,0]
[null,"벽체 PUTTY",null,"줄퍼티 2회, 올퍼티 1회","M2",20.4,1,null,0,null,0,0]
[null,"벽체 수성도장",null,"지정칼라","M2",20.4,1,null,0,null,0,0]
[null,"부자재",null,null,"식",1,1,null,0,null,0,0]
[]
[null,"<바닥 공사>"]
[null,"모노륨 1.8T",null,null,"M2",54.285,1.2,null,0,null,0,0]
[null,"부자재",null,null,"식",1,1,null,0,null,0,0]
[]
[null,"합       계",{"$nulls":6},0,null,0,0]
[]
["9","설비공사"]
[null,"<위생 배관 공사>"]
[null,"PVC-PIPE(VG1)",null,"75A","M",54,1,null,0,null,0,0]
[null,"PVC-PIPE(VG1)",null,"50A","M",20,1,null,0,null,0,0]
[null,"PVC-YT(DTS)",null,"100A","EA",2,1,null,0,null,0,0]
[null,"PVC-YT(DTS)",null,"75A","EA",8,1,null,0,null,0,0]
[null,"PVC-YT(DTS)",null,"50A","EA",8,1,null,0,null,0,0]
[null,"PVC-ELBOW(DTS)",null,"75A","EA",6,1,null,0,null,0,0]
[null,"PVC-ELBOW(DTS)",null,"50A","EA",20,1,null,0,null,0,0]
[null,"PVC-소제구",null,"75A","EA",7,1,null,0,null,0,0]
[null,"PVC-소켓",null,"75A","EA",4,1,null,0,null,0,0]
[null,"관행거(달대볼트)",null,"75A","개소",14,1,null,0,null,0,0]
[null,"관행거(달대볼트)",null,"50A","개소",5,1,null,0,null,0,0]
[null,"배관용 스테인리스강관",null,"20A","M",136,1,null,0,null,0,0]
[null,"배관용 스테인리스강관",null,"15A","M",42,1,null,0,null,0,0]
[null,"관보온(아티론,매직)",null,"20TxD20","M",136,1,null,0,null,0,0]
[null,"관보온(아티론,매직)",null,"20TxD15","M",42,1,null,0,null,0,0]
[null,"STS관 이음쇠(죠인트식)",null,"엘보(SR-JOINT) 13SU","EA",64,1,null,0,null,0,0]
[null,"STS관 이음쇠(죠인트식)",null,"엘보(SR-JOINT) 20SU","EA",18,1,null,0,null,0,0]
[null,"STS관 이음쇠(죠인트식)",null,"티이(SR-JOINT) D20","EA",8,1,null,0,null,0,0]
[null,"STS관 이음쇠(죠인트식)",null,"티이(SR-JOINT) D25","EA",6,1,null,0,null,0,0]
[null,"STS관 이음쇠(죠인트식)",null,"소켓(SR-JOINT) 20SU","EA",8,1,null,0,null,0,0]
[null,"STS관 이음쇠(죠인트식)",null,"M아답타소켓(SR-J) 13SU","EA",12,1,null,0,null,0,0]
[null,"STS관 이음쇠(죠인트식)",null,"M아답타소켓(SR-J) 20SU","EA",4,1,null,0,null,0,0]
[null,"STS관 이음쇠(죠인트식)",null,"M아답타소켓(SR-J) 25SU","EA",6,1,null,0,null,0,0]
[null,"STS관 이음쇠(죠인트식)",null,"M-union(SR-J) 25SU","EA",8,1,null,0,null,0,0]
[null,"STS관 이음쇠(죠인트식)",null,"수전엘보(SR-J)13*15A","EA",10,1,null,0,null,0,0]
[null,"PT닛블",null,"15A","EA",12,1,null,0,null,0,0]
[null,"PT닛블",null,"25A","EA",6,1,null,0,null,0,0]
[null,"STS 유니온",null,"25A","EA",6,1,null,0,null,0,0]
[null,"STS볼 밸브 (보온용)",null,"10kg,D20","EA",3,1,null,0,null,0,0]
[null,"STS볼 밸브 ",null,"10kg,D15","EA",10,1,null,0,null,0,0]
[null,"관붙이앵글밸브",null,"10kg,D15","EA",10,1,null,0,null,0,0]
[null,"절연행가(달대볼트)",null,"D15","개소",18,1,null,0,null,0,0]
[null,"절연행가(달대볼트)",null,"D20","개소",42,1,null,0,null,0,0]
[null,"부재료",null,"재료의3%","식",1,1,null,0,null,0,0]
[null,"노무비",null,"배관공","인",18,1,null,0,null,0,0]
[null,"노무비",null,"조력공","인",14,1,null,null,null,0,0]
[null,"공구손료",null,"노무비의3%","식",1,1,null,null,null,0,0]
[]
[null,"<공압 배관 공사>"]
[null,"동관(L-type)",null,"20A","M",284,1,null,0,null,0,0]
[null,"동엘보",null,"20A","EA",96,1,null,0,null,0,0,null,192]
[null,"동티이",null,"20A","EA",72,1,null,0,null,0,0,null,216]
[null,"동소켓",null,"20A","EA",46,1,null,0,null,0,0,null,92]
[null,"CMA",null,"20A","EA",72,1,null,0,null,0,0,null,72]
[null,"황동볼 밸브 ",null,"10kg,D20","EA",84,1,null,0,null,0,0]
[null,"절연행가(달대볼트)",null,"D20","개소",56,1,null,0,null,0,0]
[null,"동관용접",null,"20A","개소",572,1,null,0,null,0,0]
[null,"부재료",null,"재료의3%","식",1,1,null,0,null,0,0]
[null,"노무비",null,"배관공","인",36,1,null,0,null,0,0]
[null,"노무비",null,"조력공","인",18,1,null,0,null,0,0]
[null,"공구손료",null,"노무비의3%","식",1,1,null,0,null,0,0]
[]
[null,"합       계",{"$nulls":6},0,null,0,0]
[]
["10","공조 및 냉.난방 공사"]
[null,"<급. 배기 외벽, 옥상 메인덕트 공사>"]
[null,"급기 에어포일팬",null,"8,200CMH*100MMAQ*5HP","대",1,1,null,0,null,0,0]
[null,"배기 시로코팬",null,"15,000CMH*50MMAQ*10HP","대",1,1,null,0,null,0,0]
[null,"각형덕트 제작",null,"0.6T 1000*500","M2",480,1,null,0,null,0,0]
[null,"각형덕트 제작",null,"0.5T 1000*300","M2",28,1,null,0,null,0,0]
[null,"행거레일",null,"40*30","M",56,1,null,0,null,0,0]
[null,"EV펙킹",null,"30W","EA",50,1,null,0,null,0,0]
[null,"볼트너트(아연도)",null,"3/8\"*30","EA",400,1,null,0,null,0,0]
[null,"부재료",null,"재료의3%","식",1,1,null,0,null,0,0]
[null,"스카이작업차임대",null,"8톤","일",3,1,null,0,null,0,0]
[null,"외벽덕트구 컷팅,파취",null,"1000*300(화강석,옹벽)","개소",2,1,null,0,null,0,0]
[null,"노무비",null,"덕트공","인",22,1,null,0,null,0,0]
[null,"공구손료",null,"노무비의3%","식",1,1,null,0,null,0,0]
[null,"기초 콘크리트_(옥상 급.배기 브로어 설치 베이스)",null,"1000*2000*200","개소",2,1,null,0]
[]
[null,"<실내 공조공사>"]
[null,"각형덕트 제작",null,"0.5T 1000*300","M2",360,1.05,null,0,null,0,0]
[null,"덕트보온(고무발포)",null,"9t","M2",180,1,null,0,null,0,0]
[null,"행거레일",null,"40*30","M",120,1,null,0,null,0,0]
[null,"EV펙킹",null,"30W","EA",60,1,null,0,null,0,0]
[null,"볼트너트(아연도)",null,"3/8\"*30","EA",500,1,null,0,null,0,0]
[null,"MOTORZED VOLUM DAMPER",null,"400*300","EA",8,1,null,0,null,0,0]
[null,"디퓨져(각원팬)",null,"300*300*200","EA",88,1,null,0,null,0,0]
[null,"플렉시블덕트호스",null,"D200","M",120,1.05,null,0,null,0,0]
[null,"플렉시블덕트호스(보온)",null,"D200","M",120,1,null,0,null,0,0]
[null,"스텐반도",null,"D200","EA",176,1,null,0,null,0,0]
[null,"부재료",null,null,"식",1,1,null,0,null,0,0]
[null,"노무비",null,"덕트공","인",40,1,null,0,null,0,0]
[null,"노무비",null,"보온공","인",12,1,null,0,null,0,0]
[null,"공구손료",null,"노무비의3%","식",1,1,null,0,null,0,0]
[null,"T.A.B",null,null,"식",1,1,null,0,null,0,0]
[]
[null,"<자동제어 공사>"," 급.배기 자동제어 분전함 제작시 전압,전류,kw 지시계 설치(부하용량 3kw 이상 설치 적용)"]
[null,"강제전선관","  ","D16~","M",500,1,null,0,null,0,0]
[null,"전선관부속류",null,null,"식",1,1,null,0,null,0,0]
[null,"와이어",null,"제어용","M ",540,1,null,0,null,0,0]
[null,"중앙감시컴,프로그램",null,null,"식",1,1,null,0,null,0,0]
[null,"컨트롤판넬",null,"급.배기용","조",2,1,null,0,null,0,0]
[null,"FAN 인버터제어기",null,"5HP_(급기용)","조",1,1,null,0,null,0,0]
[null,"FAN 인버터제어기",null,"10HP_(배기용)","조",1,1,null,0,null,0,0]
[null,"각실 S/W BOX",null,"램프형 2구 S/W","조",4,1,null,0,null,0,0]
[null,"부재료",null,null,"식",1,1,null,0,null,0,0]
[null,"노무비",null,"계장공","인",30,1,null,0,null,0,0]
[null,"노무비",null,"조력공","인",16,1,null,0,null,0,0]
[null,"공구손료",null,"노무비의3%","식",1,1,null,0,null,0,0]
[]
[null,"<냉.난방 설비공사>","FCU 4WAY 이설 10대 / 4WAY 신설 1대"]
[null,"FCU(4-way,유,무선리모컨포함)",null,"8,000kcal/h","대",1,1,null,0,null,0,0]
[null,"배관용 스테인리스강관(ksd3595)",null,"20su","M",18,1,null,0,null,0,0]
[null,"관보온재(가교발포+매직)",null,"20Tx20A","M",20,1,null,0,null,0,0]
[null,"STS관 이음쇠(죠인트식)",null,"엘보(SR-JOINT) 20su","EA",20,1,null,0,null,0,0]
[null,"STS관 이음쇠(죠인트식)",null,"티이(SR-JOINT)25su","EA",2,1,null,0,null,0,0]
[null,"STS관 이음쇠(죠인트식)",null,"티이(SR-JOINT)40 su*25su","EA",1,1,null,0,null,0,0]
[null,"STS관 이음쇠(죠인트식)",null,"소켓(SR-JOINT)20su","EA",30,1,null,0,null,0,0]
[null,"STS관 이음쇠(죠인트식)",null,"M아답타소켓(SR-JOINT)25su","EA",1,1,null,0,null,0,0]
[null,"STS관 이음쇠(죠인트식)",null,"M아답타소켓(SR-JOINT)20su","EA",20,1,null,0,null,0,0]
[null,"STS 볼밸브 ",null,"10kg,D20","EA",20,1,null,0,null,0,0]
[null,"절연행가(달대볼트)",null,"D20","개소",20,1,null,0,null,0,0]
[null,"부재료",null,"재료의3%","대",1,1,null,0,null,0,0]
[null,"노무비",null,"배관공","인",11,1,null,0,null,0,0]
[null,"공구손료",null,"노무비의3%","대",1,1,null,0,null,0,0]
[]
[]
[null,"합          계",{"$nulls":6},0,null,0,0]