{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["원가계산서","집계표","내역서"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":23,"defined_names":124,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"원가계산서","index":0,"n_rows":28,"n_cols":7,"rows_kept":28,"cut":false,"hidden":false,"merged":[[27,1,27,3],[21,1,21,3],[22,1,22,3],[23,1,23,3],[24,1,24,3],[25,1,25,3],[26,1,26,3],[0,1,0,6],[1,1,1,4],[1,5,1,6],[2,1,2,3],[3,1,20,1],[3,2,6,2],[7,2,9,2],[10,2,20,2]],"flags":["formulas_cached_only"]}
[null," 공 사 원 가 계 산 서"]
[null,"공사명 : 부천대학교 밀레니엄관 13층 복합공간 건축공사"]
[null,"비        목",null,null,"금      액","구        성        비","비      고"]
["A1","순   공   사   원   가","재   료   비","직  접  재  료  비",null,"자재비",""]
["A2",null,null,"간  접  재  료  비",null,"",""]
["A3",null,null,"작업설, 부산물(△)",null,"",""]
["AS",null,null,"[ 소          계 ]",null,"",""]
["B1",null,"노   무   비","직  접  노  무  비",null,"인건비(노무비)",""]
["B2",null,null,"간  접  노  무  비",null,"직접노무비 * 13.0%",""]
["BS",null,null,"[ 소          계 ]",null,"",""]
[null,null,"경비","기  계  경  비"]
["C4",null,null,"산  재  보  험  료",null,"노무비 * 3.7%",""]
["C5",null,null,"고  용  보  험  료",null,"노무비 * 1.01%",""]
["C6",null,null,"국민  건강  보험료",null,"직접노무비 * 3.43%",""]
["C7",null,null,"국민  연금  보험료",null,"직접노무비 * 4.5%",""]
["C9",null,null,"노인장기요양보험료",null,"국민건강보험료 * 11.52%",""]
[null,null,null,"퇴 직 공 제 부 금 비",null,"직접노무비 * 2.3%"]
[null,null,null,"환 경 보 전 비",null,"직접공사비 * 0.3%"]
["CA",null,null,"산업안전보건관리비",null,"(재료비+직노) * 2.93%_(4천만원 이상 / 5억 미만) / (재료비+직노) * 1.86%+5,349천원"]
["CG",null,null,"기   타    경   비",null,"(재료비+노무비) * 3.5%",""]
["CS",null,null,"[ 소          계 ]",null,"",""]
["S1","        계",null,null,null,"",""]
["D1","일  반  관  리  비",null,null,null,"계 * 6.0%",""]
["D2","이              윤",null,null,null,"(노무비+경비+일반관리비) * 15.0%"]
["D9","공   급    가   액",null,null,null,"",""]
["DB","부  가  가  치  세",null,null,null,"공급가액 * 10%",""]
["DH","도      급      액",null,null,null,"",""]
["S2","총   공   사    비",null,null,null,"",""]

{"sheet":"집계표","index":1,"n_rows":37,"n_cols":16,"rows_kept":37,"cut":false,"hidden":false,"merged":[[2,0,3,0],[2,1,3,1],[2,2,3,2],[2,3,3,3],[2,4,3,4],[2,5,3,5],[2,6,3,6],[2,7,3,7],[2,8,2,9],[2,10,2,11],[2,14,3,14],[2,15,3,15],[2,12,2,13]],"flags":["formulas_cached_only"]}
[]
[null,"집계표"]
["번호","명       칭","제조사","모델 No.","규  격","단위","수  량","자재\nloss율","자 재 비",null,"인 건 비",null,"경 비",null,"합 계","비  고"]
[{"$nulls":8},"단  가","금액","단  가","금액","단  가","금액"]
[]
["■","총괄 집계표"]
[null,"직접 공사비"]
[]
["1","가설공사",null,null,null,"LOT",1,null,null,0,null,0,null,0,0]
["2","철거공사",null,null,null,"LOT",1,null,null,0,null,0,null,0,0]
["3","E/V HALL&CORRIDOR",null,null,null,"LOT",1,null,null,0,null,0,null,0,0]
["4","LOUNGE",null,null,null,"LOT",1,null,null,0,null,0,null,0,0]
["5","CONFERENCE 1",null,null,null,"LOT",1,null,null,0,null,0,null,0,0]
["6","CONFERENCE 2",null,null,null,"LOT",1,null,null,0,null,0,null,0,0]
["7","MULTI ROOM",null,null,null,"LOT",1,null,null,0,null,0,null,0,0]
["8","TOILET(M,W)",null,null,null,"LOT",1,null,null,0,null,0,null,0,0]
["9","설비공사",null,null,null,"LOT",1,null,null,0,null,0,null,0,0]
["10","공조 및 냉.난방 공사",null,null,null,"LOT",1,null,null,0,null,0,null,0,0]
["11","기타공사",null,null,null,"LOT",1,null,null,0,null,0,null,0,0]
{"$rows_empty":17}
[null,"직접공사비 계",{"$nulls":7},0,null,0,null,0,0]

{"sheet":"내역서","index":2,"n_rows":382,"n_cols":14,"rows_kept":382,"cut":false,"hidden":false,"merged":[[2,13,3,13],[2,0,3,0],[2,1,3,1],[2,2,3,2],[2,3,3,3],[2,11,2,12],[2,4,3,4],[2,9,2,10],[2,5,2,6],[2,7,2,8]],"flags":["formulas_cached_only"]}
[]
["내역서"]
["번호","명       칭","규  격","단위","수량","자 재 비",null,"인 건 비",null,"경 비",null,"합 계",null,"비  고"]
[{"$nulls":5},"단  가","금액","단  가","금액","단  가","금액","단가","금액"]
["부천대학고 밀레니엄관 13층 복합공간 건축공사"]
[]
["1","가설공사"]
[null,"먹메김",null,"M2",429.53]
[null,"내부 수평비계",null,"M2",429.53]
[null,"현장정리",null,"M2",429.53]
[null,"현장 보양",null,"M2",429.53]
[null,"E/V 보양","플로베니어","식",1]
[null,"대운반",null,"M2",429.53]
[null,"소운반",null,"M2",429.53]
[null,"준공청소",null,"M2",429.53]
[null,"가설자재 운임비","목자재 외","대",2]
[null,"폐자재 처리","1.5TON","대",2]
[]
[null,"합       계"]
[]
["2","철거공사"]
[null,"바닥 P-TILE 철거",null,"M2",333.4]
[null,"바닥 타일 철거",null,"M2",72.5]
[null,"무근 콘크리트 철거","H:180","M2",72.5]
[null,"바닥 단상 철거","H:120","M2",25.2]
[null,"벽체 마감재 철거",null,"M2",429.53]
[null,"천장 철거","텍스+골조 철거+마감재 일체","M2",429.53]
[null,"기존 내부 창호 철거",null,"M2",12.314000000000002]
[null,"기존 집기류 철거","바가구 등","M2",429.53]
[null,"폐기물 처리","건설폐재류 1.5Ton","대",8]
[null,"폐기물 처리","폐콘크리트 5Ton","대",3]
[]
[null,"합       계"]
[]
["3","E/V HALL&CORRIDOR"]
[null,"<조명>"]
[null,"멀티 2구","LED COB 15W*2 4000K","EA",13]
[null,"라인조명","LED BAR 20W 4000K","M",11.15]
[null,"LED BAR","LED 12V 15W / 각 1줄","M",25]
[null,"SMPS","12V 300W","EA",3]
[]
[null,"<벽체 공사>"]
[null,"경량 구조틀(벽체)","65*45*0.8","M2",72.8376]
[null,"금속 수벽 구조틀(벽체)","ㅁ40*40","M2",21.01]
[null,"합판 보강","9T 합판 1ply","M2",72.8376]
[null,"석고보드 ","석고보드 9.5T 1ply","M2",42.02]
[null,"흡음재","스카이비바 50T ","M2",21.01]
[null,"MDF 알판 취부","9T MDF 1PLY","M2",72.8376]
[null,"벽면 매지 몰딩",null,"M2",72.8376]
[null,"걸레받이 취부","MDF 6T 위 도장 H:50","M",24.15]
[null,"수벽 벽체 PUTTY","줄퍼티 2회,올퍼티 1회","M2",21.01]
[null,"수벽 지정도장","지정 수성 도장","M2",56.650000000000006]
[null,"계단실 방화문 도장",null,"개소",1]
[null,"필름 마감 알판 PUTTY","줄퍼티 2회","M2",72.8376]
[null,"알판 필름취부","지정필름","M2",72.8376]
[null,"점검도어 필름 취부(소화전 포함)","지정필름","식",1]
[null,"실명사인_(아크릴 스카시)",null,"개소",3]
[]
[null,"<천장공사>"]
[null,"경량 구조틀 (천장)","50*19*0.5","M2",26]
[null,"AL스크린 루바 구조틀(블랙 분체포함)","앙카,볼트, 각파이프 ","M2",26]
[null,"석고보드 ","석고보드 9.5T 2ply","M2",26]
[null,"EV HALL 천장 단짓기","갈바 1.6T 300*200","M",14]
[null,"복도 간접 등박스","갈바 1.6T 150*200*200*270*200*150*40","M",27.6]
[null,"천장 라인조성","갈바 1.6T 55*60","M",11.15]
[null,"AL스크린 루바(백색 분체 포함)","40*120 @240 (내경200)","M2",26]
[null,"AL마구리캡(백색 분체 포함)","40*120","M2",26]
[null,"천장 PUTTY","줄퍼티 2회,올퍼티 1회","M2",26]
[null,"천장 도장 작업","지정 수성 도장","M2",26]
[null,"노출천장 도장 작업","지정 수성 도장","M2",26.5]
[null,"유성도장","단짓기+등박스","M",52.75]
[]
[null,"<바닥공사>"]
[null,"경사재료 분리대","1.5T SUS H/L","M",7]
[null,"바닥 타일","600*600(갤럭시 그레이)","M2",43.37]
[null,"EV HALL 바닥 화강석 이색석재 교체","450mm*450mm","개소",7]
[]
[null,"합       계"]
[]
["4","LOUNGE"]
[null,"<조명>"]
[null,"멀티 2구","LED COB 15W*2 4000K","EA",9]
[null,"멀티 1구","LED COB 15W 4000K","EA",9]
[null,"라인등","LED 56W 4000K L: 1200","EA",24]
[null,"LED BAR","LED 12V 15W / 각 1줄","M",18.5]
[null,"SMPS","12V 300W","EA",1]
[null,"SMPS","12V 150W","EA",2]
[null,"LED T-5","LED 12V 15W / 각 1줄","M",2]
[]
[null,"<벽체 공사>"]
[null,"경량 구조틀(벽체)","65*45*0.8","M2",74.328]
[null,"합판 보강","9T 합판 1ply","M2",80.268]
[null,"석고보드 ","석고보드 9.5T 1ply","M2",79.784]
[null,"흡음재","스카이비바 50T ","M2",32.56]
[null,"MDF 취부","9T MDF 1PLY","M2",10.440000000000001]
[null,"가구 매립 게이트","D600","M",8.1]
[null,"기둥 팀버패턴 몰딩 취부","MDF 30*9","M",156.79999999999998]
[null,"벽체 경사 루바 취부","MDF 45*40*85","M",43.84]
[null,"걸레받이 취부","MDF 6T 위 도장 H:50","M",43.599999999999994]
[null,"창고 도어 신설","문틀+하드웨어 일체","조",1]
[null,"벽체 및 수벽 PUTTY","줄퍼티 2회,올퍼티 1회","M2",123.32600000000001]
[null,"수벽 지정도장","지정 수성 도장","M2",29.920000000000005]
[null,"창고벽체 지정도장",null,"M2",33.012]
[null,"벽체 스페셜 지정도장","오이코스(트라버티노)","M2",107.99000000000001]
[null,"유리 프레임","갈바 1.6T","M",23.700000000000003]
[null,"자동문 점검도어","갈바 1.6T","M",3]
[null,"자동문 하드웨어 일체",null,"SET",1]
[null,"자동도어(가마찌도어형)","790*2400","EA",2]
[null,"강화유리","12T ","자평",111]
[null,"필름면 PUTTY","줄퍼티 2회","M2",75.55704]
[null,"필름취부","지정필름","M2",75.55704]
[null,"프레임 필름 취부","지정필름","M",23.700000000000003]
[null,"붙박의 의자 구조틀",null,"M",7]
[null,"바테이블 금속 구조틀","ㅁ40*40","M",9.76]
[null,"바테이블 MDF 취부","9T MDF 1PLY","M2",9.76]
[null,"실명사인_(아크릴 스카시)",null,"개소",2]
[null,"로고사인_(비조명)",null,"개소",2]
[null,"유리 컷팅 시트",null,"개소",5]
[]
[null,"<천장공사>"]
[null,"커튼박스","갈바 1.6T 150*200","M",13.1]
[null,"단짓기","갈바 1.6T 20*200","M",12]
[null,"경량 구조틀 (천장)","50*19*0.5","M2",5.895]
[null,"AL스크린 루바 구조틀(블랙 분체포함)","앙카,볼트, 각파이프 ","M2",50.7]
[null,"석고보드 ","석고보드 9.5T 2ply","M2",5.895]
[null,"AL스크린 루바(백색 분체 포함)","40*120 @240 (내경200)","M2",22]
[null,"AL스크린 루바(우드필름 포함)","40*120 @240 (내경200)","M2",28.700000000000003]
[null,"AL마구리캡(백색 분체 포함)","40*120","M2",74]
[null,"AL마구리캡(우드필름 포함)","40*120","M2",44]
[null,"천장 PUTTY","줄퍼티 2회,올퍼티 1회","M2",5.895]
[null,"천장 도장 작업","지정 수성 도장","M2",12.125]
[null,"노출천장 도장 작업","지정 수성 도장","M2",57.345]
[null,"유성도장","단짓기+등박스","M",25.1]
[]
[null,"<바닥공사>"]
[null,"재료분리대","3T SUS 평철","M",14]
[null,"경사재료 분리대","1.5T SUS H/L","M",1]
[null,"바닥 타일","600*600(갤럭시 그레이)","M2",32.24]
[null,"바닥 타일","150*590(우드타일)","M2",31]
[null,"붙임몰탈(매지 포함)",null,"M2",100.3]
[null,"창고 P-TILE(부자재 포함)","DTE2904 450*450","M2",6.23]
[]
[null,"<가구공사>"]
[null,"하부장(인조석+쓰레기 투입구+싱크볼 포함)","2200*600*850","M",2.2]
[null,"상부장","2900*400*700","M",2.9]
[null,"파이프 선반장","2760*2400*320","M2",6.624]
[null,"붙박이 의자 쿠션","인조가죽 시트","M",7]
[null,"가구 세팅비",null,"인",3]
[]
[null,"합       계"]
[]
["5","CONFERENCE 1"]
[null,"<조명>"]
[null,"멀티 2구","LED COB 15W*2 4000K","EA",10]
[null,"원형 매입등","LED COB 25W*2 4000K","EA",5]
[]
[null,"<벽체 공사>"]
[null,"경량 구조틀(벽체)","65*45*0.8","M2",53.782000000000004]
[null,"합판 보강","9T 합판 1ply","M2",77.278]
[null,"석고보드 ","석고보드 9.5T 1ply","M2",549.2050000000002]
[null,"흡음재","스카이비바 50T ","M2",32.56]
[null,"MDF 취부(패턴 도장 면)","9T MDF 1PLY","M2",12.816]
[null,"알판 취부(패브릭면)","MDF 각면 가공","M2",44.278000000000006]
[null,"패브릭 취부",null,"M2",44.278000000000006]
[null,"패브릭 알판 금속 재료분리대","발색 SUS","M",39.300000000000004]
[null,"걸레받이 취부","MDF 6T 위 도장 H:50","M",22.900000000000002]
[null,"매입 필경대","SUS H/L","M",2]
[null,"창고 도어 신설","문틀+하드웨어 일체","조",1]
[null,"벽체 PUTTY","줄퍼티 2회,올퍼티 1회","M2",42.706]
[null,"창고벽체 지정도장",null,"M2",30.130000000000003]
[null,"벽체 지정도장","투톤","M2",12.576]
[null,"유리 프레임","갈바 1.6T","M",20.69]
[null,"플로어 힌지","K-8300","SET",1]
[null,"도어체크","K1630","SET",1]
[null,"가마찌도어","840*2365","SET",1]
[null,"가마찌도어 손잡이",null,"조",1]
[null,"프레임 필름 취부","지정필름","M",20.69]
[null,"백페인트 글라스","지정백색","자평",144]
[null,"강화유리","12T ","자평",126]
[null,"실명사인_(아크릴 스카시)",null,"개소",2]
[null,"유리 컷팅 시트",null,"개소",5]
[]
[null,"<천장공사>"]
[null,"경량 구조틀 (천장)","50*19*0.5","M2",46.58]
[null,"석고보드 ","석고보드 9.5T 2ply","M2",46.58]
[null,"멀티 2구 등박스","갈바 1.6T 200*200","M",14.4]
[null,"천장 라인조성","갈바 1.6T 40*40","M",14.4]
[null,"천장 포인트 컬러 단짓기","갈바 1.6T 50*10","M",17.6]
[null,"갈바 점검구","450*450","EA",1]
[null,"커튼 박스","갈바 위 도장","M",5.25]
[null,"빔프로젝트 스크린 박스","갈바 위 도장","M",2.26]
[null,"천장 PUTTY","줄퍼티 2회,올퍼티 1회","M2",46.58]
[null,"천장 도장 작업","지정 수성 도장","M2",52.36]
[null,"유성도장",null,"M",53.910000000000004]
[]
[null,"<바닥공사>"]
[null," CARPET-TILE(부자재 포함)","CAT9302","M2",46.58]
[null,"창고 P-TILE(부자재 포함)","DTE2904 450*450","M2",5.78]
[]
[null,"합       계"]
[]
["6","CONFERENCE 2"]
[null,"<조명>"]
[null,"멀티 2구","LED COB 15W*2 4000K","EA",15]
[null,"원형 매입등","LED COB 25W*2 4000K","EA",5]
[]
[null,"<벽체 공사>"]
[null,"경량 구조틀(벽체)","65*45*0.8","M2",41.127]
[null,"합판 보강","9T 합판 1ply","M2",64.623]
[null,"석고보드 ","석고보드 9.5T 1ply","M2",53.708000000000006]
[null,"흡음재","스카이비바 50T ","M2",32.56]
[null,"MDF 취부(패턴 도장 면)","9T MDF 1PLY","M2",12.816]
[null,"알판 취부(패브릭면)","MDF 각면 가공","M2",23.056000000000004]
[null,"패브릭 취부",null,"M2",23.056000000000004]
[null,"패브릭 알판 금속 재료분리대","발색 SUS","M",23.580000000000002]
[null,"걸레받이 취부","MDF 6T 위 도장 H:50","M",24.1]
[null,"매입 필경대","SUS H/L","M",2]
[null,"창고 도어 신설","문틀+하드웨어 일체","조",1]
[null,"벽체 PUTTY","줄퍼티 2회,올퍼티 1회","M2",42.444]
[null,"창고벽체 지정도장",null,"M2",29.868000000000002]
[null,"벽체 지정도장","투톤","M2",12.576]
[null,"유리 프레임","갈바 1.6T","M",24.740000000000002]
[null,"플로어 힌지","K-8300","SET",1]
[null,"도어체크","K1630","SET",1]
[null,"가마찌도어","840*2365","SET",1]
[null,"가마찌도어 손잡이",null,"조",1]
[null,"프레임 필름 취부","지정필름","M",24.740000000000002]
[null,"백페인트 글라스","지정백색","자평",144]
[null,"강화유리","12T ","자평",180]
[null,"실명사인_(아크릴 스카시)",null,"개소",2]
[null,"유리 컷팅 시트",null,"개소",6]
[]
[null,"<천장공사>"]
[null,"경량 구조틀 (천장)","50*19*0.5","M2",57.69]
[null,"석고보드 ","석고보드 9.5T 2ply","M2",57.69]
[null,"멀티 2구 등박스","갈바 1.6T 200*200","M",21.6]
[null,"천장 라인조성","갈바 1.6T 40*40","M",21.6]
[null,"천장 포인트 컬러 단짓기","갈바 1.6T 50*10","M",17.6]
[null,"갈바 점검구","450*450","EA",1]
[null,"커튼 박스","갈바 위 도장","M",11]
[null,"빔프로젝트 스크린 박스","갈바 위 도장","M",2.26]
[null,"천장 PUTTY","줄퍼티 2회,올퍼티 1회","M2",57.69]
[null,"천장 도장 작업","지정 수성 도장","M2",63.25]
[null,"유성도장",null,"M",74.06000000000002]
[]
[null,"<바닥공사>"]
[null," CARPET-TILE(부자재 포함)","CAT9302","M2",57.69]
[null,"창고 P-TILE(부자재 포함)","DTE2904 450*450","M2",5.56]
[]
[null,"합       계"]
[]
["7","MULTI ROOM"]
[null,"<조명>"]
[null,"원형 매입등","LED COB 25W*2 4000K","EA",82]
[null,"LED BAR","LED 12V 15W / 각 1줄","M",103.5]
[null,"SMPS","12V 200W","EA",12]
[null,"SMPS","12V 300W","EA",1]
[]
[null,"<벽체 공사>"]
[null,"경량 구조틀(벽체)","65*45*0.8","M2",126.88325]
[null,"합판 보강","9T 합판 1ply","M2",126.88325]
[null,"석고보드 ","석고보드 9.5T 1ply","M2",19.360000000000003]
[null,"라인 흡음판"," 9T","M2",83.02875]
[null,"MDF 알판 취부 _(도장 면)","9T MDF 1PLY","M2",45.6425]
[null,"걸레받이 취부","MDF 6T 위 도장 H:50","M",59.6]
[null,"매입 필경대","SUS H/L","M",2.4]
[null,"창고 도어 신설","문틀+하드웨어 일체","조",2]
[null,"분전함 점검도어","문틀+하드웨어 일체","조",1]
[null,"벽체 PUTTY","줄퍼티 2회,올퍼티 1회","M2",151.87125]
[null,"창고벽체 지정도장",null,"M2",60.78400000000001]
[null,"벽체 지정도장","투톤","M2",151.87125]
[null,"유리 프레임","갈바 1.6T","M",6.74]
[null,"가마찌도어 인방","1500*420 갈바 1.6T","M",1.5]
[null,"플로어 힌지","K-8300","SET",2]
[null,"도어체크","K1630","SET",2]
[null,"가마찌도어","870*2200","SET",1]
[null,"가마찌도어","570*2200","SET",1]
[null,"가마찌도어 손잡이",null,"조",2]
[null,"필름면 PUTTY","줄퍼티 2회","M2",41.175]
[null,"필름취부","지정필름","M2",41.175]
[null,"프레임 필름 취부","지정필름","M",6.74]
[null,"백페인트 글라스","지정백색","자평",64]
[null,"실명사인_(아크릴 스카시)",null,"개소",2]
[null,"유리 컷팅 시트",null,"개소",2]
[]
[null,"<천장공사>"]
[null,"경량 구조틀 (천장)","50*19*0.5","M2",137.10999999999999]
[null,"경량 구조틀 (천장)","T-BAR","M2",28.52]
[null,"마이톤","600*600 ","M2",26.8]
[null,"석고보드 ","석고보드 9.5T 2ply","M2",137.10999999999999]
[null,"간접 등박스 (일자)","갈바 1.6T 200*120*50","M",79.8]
[null,"간접 등박스 (라운드)","갈바 1.6T 200*120*50","개소",24]
[null,"천장 라인드퓨져 하우징조성","갈바 1.6T 50*15","M",48.9]
[null,"갈바 점검구","450*450","EA",5]
[null,"커튼 박스","갈바 위 도장","M",17.55]
[null,"빔프로젝트 스크린 박스","갈바 위 도장","M",2.26]
[null,"바텐박스 제작설치","ST'L GALVA 200*250","M",5.2]
[null,"전동 바텐","5M, 리모콘 포함","개소",1]
[]
[null,"천장 PUTTY","줄퍼티 2회,올퍼티 1회","M2",137.10999999999999]
[null,"천장 도장 작업","지정 수성 도장","M2",160.31]
[null,"유성도장",null,"M",177.51]
[]
[null,"<바닥공사>"]
[null,"바닥 셀프 레벨링",null,"M2",72.5]
[null," CARPET-TILE(부자재 포함)","CAT9307","M2",137.10999999999999]
[null,"창고 P-TILE(부자재 포함)","DTE2904 450*450","M2",23.1]
[null,"이동식 무대 단상","1200*1200*200","SET",8]
[]
[null,"<가구공사>"]
[null,"하부장(인조석+싱크볼 포함)","3100*600*850","M",3.1]
[null,"상부장","1110*400*550","M",2.9]
[null,"간접 선반","1870*400","M",3.74]
[null,"가구 게이트","3100*2200*600","M",7.5]
[null,"루바 슬라이딩 도어(하드웨어 포함)",null,"SET",1]
[null,"가구 세팅비",null,"인",3]
[]
[null,"합       계"]
[]
["8","TOILET(M,W)"]
[null,"<벽체 공사>"]
[null,"벽체 PUTTY","줄퍼티 2회,올퍼티 1회","M2",58.56]
[null,"벽체 지정도장","지정 수성 도장","M2",58.56]
[]
[null,"합       계"]
[]
["9","설비공사"]
[null,"<위생 배관 공사>"]
[null,"급수(온수, 냉수) 급탕 배관","(부속 자재 포함)","M",22]
[null,"배수 배관","(부속 자재 포함)","M",12]
[null,"수전","대림바스 냉온수 겸용","개소",2]
[null,"잡자재비","재료비의 3%","식",1]
[null,"인건비",null,"인",4]
[]
[null,"합       계"]
[]
["10","공조 및 냉.난방 공사"]
[null,"<공조공사>"]
[null,"전열교환기","SW-1000SH","대",1]
[null,"라인 디퓨져","L1,200*ND150","조",10]
[null,"원형 디퓨져","D300*ND150","조",38]
[null,"스파이럴 덕트","D250","M",24]
[null,"스파이럴 덕트 행거(달대볼트)","D250","개소",24]
[null,"플렉시볼덕트호스(보온)","D250","M",15]
[null,"플렉시볼덕트호스","D150","M",80]
[null,"스파이럴 덕트 Y","D250","EA",12]
[null,"스텐밴드","150*250","EA",36]
[null,"후드캡(STS)","D250","EA",2]
[null,"부재료","재료비의 3%","식",1]
[null,"노무비","덕트공","인",10]
[null,"공구손료","노무비의3%","식",1]
[]
[null,"<냉.난방 설비공사>"]
[null,"RPUW241X9H (실외기)","24마력(한랭지형)","대",1]
[null,"RNW1100A2U (실내기)","30평형 (컨퍼런스2)","대",1]
[null,"RNW1000A2U (실내기)","28평형 (컨퍼런스1)","대",1]
[null,"RNW0720A2U (실내기)","18평형 (라운지2대,멀티룸4대)","대",6]
[null,"설치비",null,"대",8]
[null,"배관공사 ",null,"대",8]
[null,"드레인공사",null,"대",8]
[null,"유선리모컨",null,"대",8]
[null,"분기관",null,"대",7]
[null,"실외기 받침대",null,"대",1]
[null,"기밀 및 냉매충전",null,"대",1]
[null,"pc제어",null,"대",1]
[null,"배관트레이",null,"M",95]
[null,"실외기 양중","100Ton 크레인","회",1]
[]
[null,"합       계"]
[]
["11","기타공사"]
[null,"<블라인드 공사>"]
[null,"우드 블라인드","방염 지정우드","M2",63.540000000000006]
[]
[null,"<외창 프레임 필름 공사>"]
[null,"씰링 제거",null,"M",208.5]
[null,"프레임 필름 취부","방염 외부창호용 필름","M",163.5]
[null,"잡자재비","재료비의 3%","식",1]
[null,"재씰링","다우코닝 구조용 실리콘","M",208.5]
[]
[]
[null,"합       계"]