{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["원가계산서","집계표","내역서"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":23,"defined_names":123,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"원가계산서","index":0,"n_rows":30,"n_cols":7,"rows_kept":30,"cut":false,"hidden":false,"merged":[[29,1,29,3],[22,1,22,3],[23,1,23,3],[24,1,24,3],[26,1,26,3],[27,1,27,3],[28,1,28,3],[25,1,25,3],[0,1,0,6],[1,1,1,4],[1,5,1,6],[2,1,2,3],[3,1,21,1],[3,2,6,2],[7,2,9,2],[10,2,21,2]],"flags":["formulas_cached_only"]}
[null," 공 사 원 가 계 산 서"]
[null,"공사명 : 부천대학교 몽당도서관 창의복합 문화공간 건축공사"]
[null,"비        목",null,null,"금      액","구        성        비","비      고"]
["A1","순   공   사   원   가","재   료   비","직  접  재  료  비",null,"자재비",""]
["A2",null,null,"간  접  재  료  비",null,"",""]
["A3",null,null,"작업설, 부산물(△)",null,"",""]
["AS",null,null,"[ 소          계 ]",null,"",""]
["B1",null,"노   무   비","직  접  노  무  비",null,"인건비(노무비)",""]
["B2",null,null,"간  접  노  무  비",null,"직접노무비 * 13.0%",""]
["BS",null,null,"[ 소          계 ]",null,"",""]
[null,null,"경비","기   계    경   비"]
["C4",null,null,"산  재  보  험  료",null,"노무비 * 3.7%",""]
["C5",null,null,"고  용  보  험  료",null,"노무비 * 1.01%",""]
["C6",null,null,"국민  건강  보험료",null,"직접노무비 * 3.495%","1개월 미만 미적용"]
["C7",null,null,"국민  연금  보험료",null,"직접노무비 * 4.5%","1개월 미만 미적용"]
["C9",null,null,"노인장기요양보험료",null,"국민건강보험료 * 12.27%","1개월 미만 미적용"]
["CA",null,null,"산업안전보건관리비",16864542,"(재료비+직노) * 1.86%+5,349천원","5억이상으로 수식적용"]
[null,null,null,"퇴 직 공 제 부 금 비",4691910,"직접노무비 * 2.3%"]
[null,null,null,"환  경  보  전  비",null,"직접공사비 * 0.3%"]
[null,null,null,"건설기계대여금지급보증서발급수수료",null,"직접공사비 * 0.1%"]
["CG",null,null,"기   타    경   비",null,"(재료비+노무비) * 5.8%",""]
["CS",null,null,"[ 소          계 ]",null,"",""]
["S1","        계",null,null,null,"",""]
["D1","일  반  관  리  비",null,null,null,"계 * 6.0%",""]
["D2","이              윤",null,null,null,"(노무비+경비+일반관리비) * 15.0%",""]
[null,"단   수    정   리"]
["D9","공   급    가   액",null,null,null,"",""]
["DB","부  가  가  치  세",null,null,null,"공급가액 * 10%",""]
["DH","도      급      액",null,null,null,"",""]
["S2","총   공   사    비",null,null,null,"",""]

{"sheet":"집계표","index":1,"n_rows":36,"n_cols":13,"rows_kept":36,"cut":false,"hidden":false,"merged":[[2,12,3,12],[2,0,3,0],[2,1,3,1],[2,2,3,2],[2,3,3,3],[2,9,2,10],[2,4,3,4],[2,5,2,6],[2,7,2,8],[2,11,3,11]],"flags":["formulas_cached_only"]}
[]
[null,"집계표"]
["번호","명       칭","규  격","단위","수  량","자 재 비",null,"인 건 비",null,"경 비",null,"합 계","비  고"]
[{"$nulls":5},"단  가","금액","단  가","금액","단  가","금액"]
[]
["■","총괄 집계표"]
[null,"직접 공사비"]
[]
["1","가설공사",null,"LOT",1,null,0,null,0,null,0,0]
["2","철거공사",null,"LOT",1,null,0,null,0,null,0,0]
["3","도서관 입구 로비(입구, 방풍실)",null,"LOT",1,null,0,null,0,null,0,0]
["4","HALL",null,"LOT",1,null,0,null,0,null,0,0]
["5","인포메이션 & CAFFTERIA",null,"LOT",1,null,0,null,0,null,0,0]
["6","공용 휴식공간",null,"LOT",1,null,0,null,0,null,0,0]
["7","북카페",null,"LOT",1,null,0,null,0,null,0,0]
["8","4인 공용 학습공간",null,"LOT",1,null,0,null,0,null,0,0]
["9","공용학습공간 & 1인학습공간 ",null,"LOT",1,null,0,null,0,null,0,0]
["10","행정실 & 창고 & 도서관장실 & 회의실",null,"LOT",1,null,0,null,0,null,0,0]
["11","공통공사",null,"LOT",1,null,0,null,0,null,0,0]
{"$rows_empty":16}
[null,"직접공사비 계",{"$nulls":4},0,null,0,null,0,0]

{"sheet":"내역서","index":2,"n_rows":360,"n_cols":15,"rows_kept":360,"cut":false,"hidden":false,"merged":[[2,14,3,14],[2,0,3,0],[2,1,3,1],[2,2,3,2],[2,13,3,13],[2,3,3,3],[2,12,3,12],[4,0,4,1],[2,4,3,4],[2,5,3,5],[2,6,2,7],[2,8,2,9],[2,10,2,11]],"flags":["formulas_cached_only"]}
[]
["내역서"]
["번호","명       칭","규  격","단위","수량","자재\nloss율","자 재 비",null,"인 건 비",null,"경 비",null,"단 가","합 계","비  고"]
[{"$nulls":6},"단  가","금액","단  가","금액","단  가","금액"]
["부천대학교 몽당도서관 2층 환경개선공사"]
[]
["1","가설공사"]
[]
[null,"현장 보양",null,"M2",1186.685,1]
[null,"현장정리",null,"M2",1186.685,1]
[null,"자재양중","대.소운반","M2",1186.685,1]
[null,"준공청소",null,"M2",1186.685,1]
[null,"실리콘 마감",null,"M2",1186.685,1]
[null,"폐기물 처리","2.5 TON","차",3,1]
[]
[null,"합       계"]
[]
["2","철거공사"]
[]
[null,"도서관 입구 석재 바닥 철거","화강석 바닥","M2",119.04,1]
[null,"유리 및 SUS 후레임 철거",null,"M2",157.198,1]
[null,"내부 조적 벽체 철거",null,"M2",74.0675,1]
[null,"천장 철거","골조 철거","M2",1186.685,1]
[null,"기존 외부 창호 철거",null,"개소",44,1]
[null,"기존 집기류 철거","가구 비품 등","식",1,1]
[null,"장비임대","3.5톤 굴절 스카이","대",1,1]
[null,"혼합 폐기물 ","1.5 TON","차",10,1]
[null,"석재 폐기물 ","2.5 TON","차",10,1]
[]
[null,"합       계"]
[]
["3","도서관 입구 로비(입구, 방풍실)"]
[null,"<조명공사>"]
[null,"라인조명","LED L:2,000","EA",8,1]
[null,"라인조명","LED L:1,500","EA",8,1]
[null,"매직보드 간접조명","LED BAR","M",6.07,1]
[null,"SMPS","SMPS","개소",1,1]
[]
[null,"<벽체 공사>"]
[null,"경량 구조틀(벽체)","65*45*0.8","M2",55.151250000000005,1]
[null,"합판 보강","9T 합판 1ply","M2",55.151250000000005,1]
[null,"석고보드 ","석고보드 9.5T 1ply","M2",55.151250000000005,1]
[null,"라왕각재 ","ㅁ30*30 라왕각재","M",589.75,1]
[null,"붙박이 의자 구조틀","목재 위 지정 필름 마감","M",5.29,1]
[null,"라왕목재 의자 구조틀","ㅁ30*30 각파이프 밴딩","M",32,1]
[null,"매직보드 간접 박스","갈바 1.2T 위 지정도장","M",6.07,1]
[null,"걸레받이 취부","갈바 1.2T","M",21.01,1]
[null,"유리 프레임","SUS H/L 1.2T","M",42.806000000000004,1]
[null,"강화유리","12T ","자평",255,1]
[null,"강화도어_부속자재 포함",null,"SET",4,1]
[null,"강화도어_손잡이",null,"EA",4,1]
[null,"자동문 SET",null,"SET",1,1]
[null,"벽체 PUTTY","줄퍼타 2회,올퍼티 1회","M2",55.151250000000005,1]
[null,"벽체 지정도장","지정 수성 도장","M2",55.151250000000005,1]
[null,"걸레받이 지정 도장","지정 수성 도장","M",21.01,1]
[null,"실명 로고","H:400/15자 아크릴 스카시","개소",1,1,{"$nulls":8},"MONGDANG LIBRARY"]
[]
[null,"<천장공사>"]
[null,"경량 구조틀 (천장)","50*19*0.5","M2",119.04,1]
[null,"석고보드 ","석고보드 9.5T 2ply","M2",119.04,1]
[null,"라왕각재 ","ㅁ30*30 라왕각재","M",409.68,1]
[null,"벽체 커튼 박스","갈바 위 도장","M",10.98,1]
[null,"천장 PUTTY","줄퍼타 2회,올퍼티 1회","M2",119.04,1]
[null,"천장 도장 작업","지정 수성 도장","M2",119.04,1]
[null,"유성도장",null,"M",10.98,1]
[null,"우드 블라인드","방염 지정우드","M2",24.842250000000003,1]
[]
[null,"<바닥공사>"]
[null,"바닥 포세린 타일","600*1200 10T 지정색상","M2",119.04,1]
[null,"부자재",null,"M2",119.04,1]
[]
[null,"합       계"]
[]
["4","HALL"]
[null,"<조명공사>"]
[null,"LED BAR","LED 12V 15W / 각 2줄","M",132.6,1]
[null,"SMPS",null,"EA",26,1]
[]
[null,"<벽체 공사>"]
[null,"경량 구조틀(벽체)","65*45*0.8","M2",94.9972,1]
[null,"합판 보강","9T 합판 1ply","M2",94.9972,1]
[null,"지정템바보드","템바보드 9T","M2",94.9972,1]
[null,"원형 바테이블_지정필름마감","각파이프 위 갈바 마감","M",7.2,1]
[null,"BESTSELLER_책장","지정 필름마감 3600*1800","식",1,1]
[null,"걸레받이 취부","갈바 1.2T ","M",35.848000000000006,1]
[null,"템바 보드 위 도장마감","지정 수성 도장","M2",94.9972,1]
[null,"걸레받이 도장",null,"M",35.848000000000006,1]
[null,"로고 스카시","H:400/32자 아크릴 스카시","개소",1,1,{"$nulls":8},"BUCHEON UNIVERSITY MONGDANG LIBRARY"]
[]
[null,"<천장공사>"]
[null,"알루미늄 루바 파이프 보강","30*30 각파이프","M2",92.31,1,{"$nulls":8},"부자재 및 운반비 포함"]
[null,"알루미늄 루바 ","알루미늄 루바 레핑 50*100","M",127.49999999999999,1,{"$nulls":8},"부자재 및 운반비 포함"]
[null,"알루미늄 루바 아크릴","W: 100 화산 아크릴","M",132.6,1]
[null,"노출 천장 도장 작업","지정 수성 도장","M2",92.31,1]
[null,"유성도장",null,"M",92.31,1]
[]
[null,"합       계"]
[]
["5","인포메이션 & CAFFTERIA"]
[null,"<조명공사>"]
[null,"평판등","LED 600*600","EA",13,1]
[null,"매입등","원형 매입등","EA",9,1]
[null,"LED BAR","LED 12V 15W / 각 2줄","M",6.1,1]
[null,"SMPS",null,"EA",1,1]
[null,"투광기",null,"EA",4,1]
[]
[null,"<벽체 공사>"]
[null,"경량 구조틀(벽체)","65*45*0.8","M2",79.0495,1]
[null,"합판 보강","9T 합판 1ply","M2",100.77949999999998,1]
[null,"석고보드 ","석고보드 9.5T 1ply","M2",28.964499999999997,1]
[null,"지정템바보드","템바보드 9T","M2",49.55499999999999,1]
[null,"알판 마감","MDF 9T","M2",43.459999999999994,1]
[null,"벽체 파이프 마감","ㅁ15*15","M2",89.8199,1]
[null,"걸레받이 취부","갈바 1.2T","M",10.8,1]
[null,"벽체 PUTTY","줄퍼타 2회,올퍼티 1회","M2",28.964499999999997,1]
[null,"벽체 지정도장","지정 수성 도장","M2",78.5195,1]
[null,"유성도장",null,"M",89.8199,1]
[null,"벽체 도장마감",null,"M2",49.55499999999999,1]
[null,"전면 BAR","필름 위 인조대리석 10410*900*920","M",10.41,1]
[null,"후면 수납장","필름 위 인조대리석 8100*300*920","M",8.1,1]
[null,"SELF CARETERIA BAR","필름 위 인조대리석 6850*670*920","M",6.85,1]
[null,"선반","필름 마감 6100*320*50","M",6.1,1]
[null,"벽체 필름마감","pw","M2",43.459999999999994,1]
[null,"인포메이션 로고 스카시","H:400/11자 아크릴 스카시","개소",1,1,{"$nulls":8},"INFORMATION"]
[null,"카페테리아 로고 스카시","H:400/19자 아크릴 스카시","개소",1,1,{"$nulls":8},"MONGDANG LIBRARY CAFÉ"]
[null,"실명 로고","H: 150 아크릴 스카시","개소",1,1]
[]
[null,"<천장공사>"]
[null,"경량 구조틀 (천장)","50*19*0.5","M2",113.56,1]
[null,"석고보드 ","석고보드 9.5T 2ply","M2",113.56,1]
[null,"금속 구조틀","ㅁ15*15 각파이프","M2",52,1]
[null,"천장 PUTTY","줄퍼타 2회,올퍼티 1회","M2",113.56,1]
[null,"천장 도장 작업","지정 수성 도장","M2",113.56,1]
[]
[null,"합       계"]
[]
["6","공용 휴식공간"]
[null,"<조명공사>"]
[null,"지정 팬던트",null,"EA",24,1]
[null,"1구 사각 매입등",null,"EA",4,1]
[]
[null,"<벽체 공사>"]
[null,"경량 구조틀(벽체)","65*45*0.8","M2",74.0675,1]
[null,"합판 보강","9T 합판 1ply","M2",74.0675,1]
[null,"알판 시공","MDF 9T","M2",14.045,1]
[null,"책장","지정 필름 마감 H:2500","자",103,1]
[null,"바테이블","지정 무늬목 마감","M",5,1]
[null,"걸레받이 취부","갈바 1.2T","M",5.3,1]
[null,"벽체 PUTTY","줄퍼타 2회,올퍼티 1회","M2",14.045,1]
[null,"벽체 지정 필름","pw","M2",14.045,1]
[null,"로고 스카시","H:400/5자 아크릴 스카시","개소",1,1,{"$nulls":8},"도서검색대"]
[null,"실명 로고","H: 150 아크릴 스카시","개소",1,1]
[]
[null,"<천장공사>"]
[null,"경량 구조틀 (천장)","50*19*0.5","M2",132.48600000000002,1]
[null,"석고보드 ","석고보드 9.5T 2ply","M2",132.48600000000002,1]
[null,"천장 PUTTY","줄퍼타 2회,올퍼티 1회","M2",132.48600000000002,1]
[null,"천장 도장 작업","지정 수성 도장","M2",214.98600000000002,1]
[null,"우드 블라인드","방염 지정우드","M2",19.009999999999998,1]
[]
[null,"합       계"]
[]
["7","북카페"]
[null,"<조명공사>"]
[null,"라인조명","LED L:1800","EA",18,1]
[]
[null,"<벽체 공사>"]
[null,"경량 구조틀(벽체)","65*45*0.8","M2",119.25,1]
[null,"합판 보강","9T 합판 1ply","M2",119.25,1]
[null,"석고보드 ","석고보드 9.5T 1ply","M2",20.8025,1]
[null,"지정 흡음 보드","라인 흡읍 보드 9T","M2",83.74,1]
[null,"걸레받이 취부","SUS H/L 10*50","M",45,1]
[null,"유리 프레임","갈바 1.2T","M",10.1,1]
[null,"폴딩도어","W: 835","개소",6,1]
[null,"블랙 글라스 유리",null,"자평",270,1]
[null,"벽체 PUTTY","줄퍼타 2회,올퍼티 1회","M2",83.74,1]
[null,"책장","지정 필름 마감 H:2500","자",41,1]
[null,"붙박이 의자 구조틀","지정 필름 마감 ","M",15.8,1]
[null,"부스쇼파",null,"M",15.8,1]
[null,"유성도장",null,"M",10.1,1]
[null,"실명 로고","H: 150 아크릴 스카시","개소",1,1]
[]
[null,"<천장공사>"]
[null,"경량 구조틀 (천장)","50*19*0.5","M2",94.016,1]
[null,"석고보드 ","석고보드 9.5T 2ply","M2",94.016,1]
[null,"벽체 커튼 박스","갈바 위 도장","M",16.5,1]
[null,"루바 천장 보강","ㅁ 30*30 각파이프","M2",80.5,1]
[null,"등박스","L:1800","M",18,1]
[null,"알루미늄 루바","50*100 지정 필름마감","M",321.31,1]
[null,"천장 PUTTY","줄퍼타 2회,올퍼티 1회","M2",94.016,1]
[null,"천장 도장 작업","지정 수성 도장","M2",174.51600000000002,1]
[null,"우드 블라인드","방염 지정우드","M2",7.199999999999999,1]
[]
[null,"합       계"]
[]
["8","4인 공용 학습공간"]
[null,"<조명공사>"]
[null,"라인등","LED 56W 4000K L: 1000","EA",16,1]
[null,"2구매입등",null,"EA",11,1]
[]
[null,"<벽체 공사>"]
[null,"경량 구조틀(벽체)","65*45*0.8","M2",78.44,1]
[null,"합판 보강","9T 합판 1ply","M2",78.44,1]
[null,"석고보드","석고보드 9.5T 1ply","M2",23.32,1]
[null,"MDF_알판","MDF9T 1ply","M2",117.76599999999999,1]
[null,"걸레받이 취부","SUS H/L 10*50","M",53.239999999999995,1]
[null,"벽체 PUTTY","줄퍼타 2회,올퍼티 1회","M2",141.08599999999998,1]
[null,"벽체 지정도장","지정 수성 도장","M2",78.44,1]
[null,"벽체 지정필름마감","pw","M2",117.76599999999999,1]
[null,"하부 유리 후레임","SUS H/L ","M",9.2,1]
[null,"12T 강화유리",null,"자평",96,1]
[null,"실명 로고","H: 150 아크릴 스카시","개소",1,1]
[null,"붙박이 의자 구조틀","목대위 지정 필름 위 쇼파","M",27.04,1]
[null,"부스쇼파_W1800",null,"개소",14,1]
[null,"부스쇼파_W1300",null,"개소",2,1]
[null,"테이블",null,"개소",8,1]
[]
[null,"<천장공사>"]
[null,"경량 구조틀 (천장)","50*19*0.5","M2",115.66799999999999,1]
[null,"석고보드 ","석고보드 9.5T 2ply","M2",115.66799999999999,1]
[null,"사선 천장 구조틀 및 MDF",null,"M2",38.08,1]
[null,"천장 PUTTY","줄퍼타 2회,올퍼티 1회","M2",153.748,1]
[null,"사선 천장 필름 마감","pw","M2",38.08,1]
[null,"천장 도장 작업","지정 수성 도장","M2",115.66799999999999,1]
[]
[null,"합       계"]
[]
["9","공용학습공간 & 1인학습공간 "]
[null,"<조명공사>"]
[null,"레일",null,"M",145.92000000000002,1]
[null,"라인등","LED 23W 4000K L:1500","M",39,1]
[]
[null,"<벽체 공사>"]
[null,"경량 구조틀(벽체)","65*45*0.8","M2",207.43,1]
[null,"합판 보강","9T 합판 1ply","M2",207.43,1]
[null,"알판 취부","MDF 9T","M2",49.84650000000001,1]
[null,"지정템바보드","템바보드 9T","M2",22.26,1]
[null,"걸레받이 취부","SUS H/L 10*50","M",18.810000000000006,1]
[null,"금속 파티션 골조","30*30 각파이프","M2",84.24,1]
[null,"금속 파티션 갈바취부","1.2T 갈바절곡","M2",168.48,1]
[null,"금속 파티션 필름취부","지정 필름","M2",168.48,1]
[null,"금속 파티션 필름취부","지정 필름","M2",168.48,1]
[null,"파티션 고정식 책상","목대 위 필름 마감","개소",24,1]
[null,"유리후레임","SUS H/L 100*30","M",8.86,1]
[null,"강화유리","12T ","자평",15.2,1]
[null,"강화도어_부속자재 포함",null,"SET",1,1]
[null,"강화도어_손잡이, 플로어힌지",null,"EA",1,1]
[null,"방화 포켓도어_부속자재 포함","1900*2200","SET",1,1]
[null,"벽체 PUTTY","줄퍼타 2회,올퍼티 1회","M2",49.84650000000001,1]
[null,"벽체 필름 마감","pw","M2",49.84650000000001,1]
[null,"템바 보드위 지정 도장마감","지정 수성 도장","M2",22.26,1]
[null,"로고 스카시","H: 400/8자 아크릴 스카시","개소",1,1,{"$nulls":8},"MON GDANG"]
[null,"로고 스카시","H: 400/9자 아크릴 스카시","개소",1,1,{"$nulls":8},"STUDY CAFE"]
[null,"실명 로고","H: 150 아크릴 스카시","개소",1,1]
[null,"책장 로고","H: 150 아크릴 스카시","개소",10,1]
[null,"책장","지정 필름 마감 H:2500","자",150.2,1]
[]
[null,"<천장공사>"]
[null,"경량 구조틀 (천장)","50*19*0.5","M2",102.9636,1]
[null,"석고보드 ","석고보드 9.5T 2ply","M2",102.9636,1]
[null,"금속 구조틀","ㅁ30*30","M",145.92000000000002,1]
[null,"벽체 커튼 박스","갈바 위 도장","M",13.2,1]
[null,"천장 PUTTY","줄퍼타 2회,올퍼티 1회","M2",102.9636,1]
[null,"천장 도장 작업","지정 수성 도장","M2",102.9636,1]
[null,"유성도장",null,"M",145.92000000000002,1]
[null,"우드 블라인드","방염 지정우드","M2",19.799999999999997,1]
[]
[null,"합       계"]
[]
["10","행정실 & 창고 & 도서관장실 & 회의실"]
[null,"<조명공사>"]
[null,"원형 매입등","원형 매입등","EA",39,1]
[]
[null,"<벽체 공사>"]
[null,"경량 구조틀(벽체)","65*45*0.8","M2",207.89249999999998,1]
[null,"합판 보강","9T 합판 1ply","M2",311.11,1]
[null,"석고보드 ","석고보드 9.5T 1ply","M2",311.11,1]
[null,"걸레받이 취부","갈바 1.2T","M",117.4,1]
[null,"벽체 PUTTY","줄퍼타 2회,올퍼티 1회","M2",388.11,1]
[null,"벽체 지정도장","지정 수성 도장","M2",388.11,1]
[null,"유리 프레임","갈바 1.2T","M",23.65,1]
[null,"강화유리","12T ","자평",45,1]
[null,"강화도어_부속자재 포함",null,"SET",3,1]
[null,"강화도어_손잡이",null,"EA",3,1]
[null,"행정실 높은 책장","지정 필름 마감 H:2500","자",16,1]
[null,"행정실 낮은 책장","지정 필름 마감","자",18,1]
[null,"행정실 수납장","지정 필름 마감 및 인조대리석","자",12,1]
[null,"도서관장실_옷장","지정 필름 마감","자",8,1]
[null,"도서관장실_낮은 책장","지정 필름 마감","자",8,1]
[null,"회의실_낮은 책장","지정 필름 마감","자",9,1]
[null,"그라데이션 시트","H: 1500 그라데이션 시트","M",2.4,1]
[null,"실명 로고","H: 150 아크릴 스카시","개소",4,1]
[]
[null,"<천장공사>"]
[null,"경량 구조틀 (천장)","T-BAR","M2",149.7,1]
[null,"석고보드 ","석고보드 9.5T 2ply","M2",149.7,1]
[null,"무석면 흡음텍스","마이텍스 12mm","M2",27.84,1]
[null,"벽체 커튼 박스","갈바 위 도장","M",7.300000000000001,1]
[null,"천장 도장 작업","지정 수성 도장","M2",149.7,1]
[null,"유성도장",null,"M",7.300000000000001,1]
[null,"우드 블라인드","방염 지정우드","M2",10.83,1]
[]
[null,"합       계"]
[]
[]
["11","공통공사"]
[]
[null,"<에어컨공사>"]
[null,"-신설"]
[null,"실외기(LG전자 휘센)","34마력(한랭지형)","대",2,1]
[null,"실내기(LG전자 휘센)","40평형","대",1,1,{"$nulls":8},"카페테리아"]
[null,"실내기(LG전자 휘센)","36평형","대",6,1,{"$nulls":8},"컴퍼/휴식/방풍/4인공유"]
[null,"실내기(LG전자 휘센)","30평형","대",6,1,{"$nulls":8},"4인/공유학습/1인"]
[null,"실내기(LG전자 휘센)","28평형","대",1,1,{"$nulls":8},"행정실"]
[null,"실내기(LG전자 휘센)","18평형","대",1,1,{"$nulls":8},"도서관장실"]
[null,"실내기(LG전자 휘센)","10평형","대",1,1,{"$nulls":8},"회의실"]
[null,"설치비","실외기 2대, 실내기 17대","대",18,1]
[null,"입상 관공사",null,"대",1,1]
[null,"배관공사",null,"대",16,1]
[null,"드레인공사",null,"대",16,1]
[null,"유선리모콘",null,"대",16,1]
[null,"분기관",null,"대",16,1]
[null,"실외기 조인트",null,"대",2,1]
[null,"실외기 받침대",null,"대",2,1]
[null,"기밀 및 냉매충전",null,"식",1,1]
[null,"PC제어",null,"식",1,1]
[null,"배관트레이",null,"식",1,1]
[null,"실외기 양중","3층 옥상","식",1,1]
[]
[null,"<설비공사>"]
[null,"배관자재비",null,"식",1,1]
[null,"부자재비",null,"식",1,1]
[null,"코아타공(바닥 슬라브)","D50","개소",1,1]
[null,"시공임",null,"인",2,1]
[]
[null,"<공조공사>"]
[null,"전열교환기","SW-1000SH","대",2]
[null,"원형 디퓨져","D300*ND150","조",152]
[null,"스파이럴 덕트","D250","M",96]
[null,"스파이럴 덕트 행거(달대볼트)","D250","개소",96]
[null,"플렉시볼덕트호스(보온)","D250","M",60]
[null,"플렉시볼덕트호스","D150","M",280]
[null,"스파이럴 덕트 Y","D250","EA",48]
[null,"스텐밴드","150*250","EA",144]
[null,"후드캡(STS)","D250","EA",4]
[null,"부재료","재료비의 3%","식",1]
[null,"노무비","덕트공","인",18]
[null,"공구손료","노무비의3%","식",1]
[]
[null,"<창호공사>"]
[null,"단열 알루미늄 창호","600*1500","개소",44,1]
[null,"실리콘 마감",null,"M",370,1]
[null,"장비임대","3.5톤 굴절 스카이","대",3,1]
[]
[null,"<바닥공사>"]
[null,"바닥 데코타일",null,"M2",988.84,1]
[null,"바닥 카펫타일",null,"M2",106.66,1,{"$nulls":8},"북카페"]
[null,"OA Floor 바닥공사",null,"M2",1067.66,1]
[]
[null,"합          계"]