{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["원가계산서","집계표","상세내역서"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":15,"defined_names":1050,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"원가계산서","index":0,"n_rows":38,"n_cols":5,"rows_kept":38,"cut":false,"hidden":false,"merged":[[36,0,36,1],[37,0,37,1],[35,0,35,1],[0,0,0,4],[1,0,1,4],[4,0,7,0],[8,0,10,0],[11,0,27,0],[34,0,34,4]]}
["공 사 원 가 계 산 서"]
[" "]
["PROJECT: ","부천대학교 한길체육관 1층 샤워실 보수공사"]
["항목","구       분","금       액","구성비","비       고"]
["재료비","직접   재료비"]
[null,"간접   재료비"]
[null,"작업설부산물"]
[null,"소         계",{"$f":"SUM(C5:C7)","v":0}]
["노무비","직접노무비"]
[null,"간접노무비",null,"(직노) * 7.9%"]
[null,"소         계",{"$f":"SUM(C9:C10)","v":0}]
["경비","산출   경비",null,"내역서 경비 항목"]
[null,"근재보험료",null,"(직노) * 1%"]
[null,"영업배상보험료",null,"(직노) * 2%"]
[null,"산재보험료",null,"(노무비) * 4.05%"]
[null,"고용보험료",null,"(노무비) * 0.87%(7등급)"]
[null,"건강보험료",null,"(직노) * 1.7%","1개월 이상시 적용"]
[null,"연금보험료",null,"(직노) * 2.49%","1개월 이상시 적용"]
[null,"노인장기요양보험료",null,"(건강보험료) * 7.38%","1개월 이상시 적용"]
[null,"퇴직공제부금비",null,"(직노) * 2.3%"]
[null,"산업안전보건관리비",null,"(재료비+직노) * 1.85%"]
[null,"기타   경비",null,"(재료비+노무비) * 5.5%"]
[null,"환경보전비",null,"(재료비+직노+산출경비) * 0.3%"]
[null,"보험및 보증수수료"]
[]
[]
[]
[null,"소         계",{"$f":"SUM(C12:C26)","v":0}]
[null,"순공사원가계",{"$f":"+C8+C11+C28","v":0},"재료비+노무비+경비"]
[null,"일반관리비",{"$f":"C29*5%","v":0},"순공사원가계 * 6.0%"]
[null,"이윤",{"$f":"C29*8%","v":0},"순공사원가계 * 15.0%"]
[]
[]
[null,"합         계",{"$f":"SUM(C29:C32)","v":0}]
[]
["공급가액",null,{"$f":"ROUND(C34,-5)","v":0},"단수정리"]
["부가가치세",null,{"$f":"C36*10%","v":0},"공급가액 * 10%"]
["합계",null,{"$f":"SUM(C36:C37)","v":0}]

{"sheet":"집계표","index":1,"n_rows":24,"n_cols":13,"rows_kept":24,"cut":false,"hidden":false,"merged":[[2,8,2,9],[2,10,2,11],[2,12,3,12],[0,4,0,6],[2,0,3,0],[2,1,3,1],[2,2,3,2],[2,3,3,3],[2,4,2,5],[2,6,2,7]]}
[{"$nulls":4},"집 계 표"]
[]
["품        명","규    격","단위","수량","재  료  비",null,"노  무  비",null,"경    비",null,"합    계",null,"비고"]
[{"$nulls":4},"단가","금액","단가","금액","단가","금액","단가","금액"]
[{"$f":"상세내역서!A5","v":"1.가설공사"}]
[{"$f":"상세내역서!A12","v":"2.철거공사"}]
[{"$f":"상세내역서!A22","v":"3.타일공사"}]
[{"$f":"상세내역서!A29","v":"4.미장공사"}]
[{"$f":"상세내역서!A34","v":"5.방수공사"}]
[{"$f":"상세내역서!A41","v":"6.금속공사"}]
[{"$f":"상세내역서!A47","v":"7.유리공사"}]
[{"$f":"상세내역서!A52","v":"8.수장공사"}]
[{"$f":"상세내역서!A56","v":"9.도장공사"}]
[{"$f":"상세내역서!A63","v":"10.기타공사"}]
{"$rows_empty":9}
["합   계",{"$nulls":4},{"$f":"SUM(F5:F23)","v":0},null,{"$f":"SUM(H5:H23)","v":0},null,{"$f":"SUM(J5:J23)","v":0},null,{"$f":"SUM(L5:L23)","v":0}]

{"sheet":"상세내역서","index":2,"n_rows":70,"n_cols":13,"rows_kept":70,"cut":false,"hidden":false,"merged":[[2,8,2,9],[2,10,2,11],[2,12,3,12],[0,2,0,7],[2,0,3,0],[2,1,3,1],[2,2,3,2],[2,3,3,3],[2,4,2,5],[2,6,2,7]]}
[null,null,"직접비 상세내역서"]
[" 공사명 : 부천대학교 한길체육관 1층 샤워실 보수공사"]
["품명","규격","단위","수량","자재비",null,"노무비",null,"경 비",null,"합 계",null,"비고"]
[{"$nulls":4},"단   가 ","금   액","단   가 ","금   액","단    가 ","금    액","단   가 ","금   액"]
["1.가설공사"]
["강관조립말비계","높이2M * 1개월","M2",56]
["건축물 현장정리",null,"M2",56]
["현장 보양(바닥 및 복도)",null,"M2",240]
["준공청소",null,"M2",56]
[]
["소   계"]
["2.철거공사"]
["트렌치 철거","바닥","M",42]
["바닥타일철거","하부 몰탈 포함","M2",58]
["벽체 타일철거","H 800mm","M2",50]
["지하 1층 상부 Girder 석고보드 철거",null,"M2",20]
["폐기물상차",null,"인",10]
["폐기물운반비",null,"차",2]
["폐기물처리비",null,"TON",5]
[]
["소   계"]
["3.타일공사"]
["도기질타일","벽'도기질타일, 일반색, 300*600*10mm, H 800mm","M2",50]
["자기질타일","자기질타일, 무유, 300*300*8~11mm","M2",58]
["도기질타일 압착붙이기","벽체, 두께 7mm(일반C, 백색줄눈)","M2",50]
["타일압착붙임(바탕 68mm+압 5mm)","바닥, 300*300(일반C, 백색줄눈)","M2",58]
[]
["소   계"]
["4.미장공사"]
["모르타르 바름","내벽, 7mm(초벌), 3.6m 이하, 레미탈 포함","M2",50]
["모르타르 바름","바닥, 68mm, 레미탈 포함","M2",58]
[]
["소   계"]
["5.방수공사"]
["우레탄도막방수","비노출 H=800mm기준, 바닥 두께 3mm","M2",108]
["수밀코킹(실리콘)","코너 및 드레인 주변","M",10]
["시멘트 액체방수","바닥","M2",58]
["시멘트 액체방수","벽 H=800mm기준","M2",50]
[]
["소   계"]
["6.금속공사"]
["타일벽코너비드설치","SUS","M",35]
["SUS 트렌치","폭 150mm * 높이 80mm","M",48]
["드레인 교체","거름망 타입(청소 관리용)","개소",4]
[]
["소   계"]
["7.유리공사"]
["지하1층 샤워실 방습거울","1000mm * 2500mm","EA",1]
["샤워실 유리 칸막이 철거 후 재설치","바닥 연결브라켓 신규 설치 기준","EA",28]
[]
["소   계"]
["8.수장공사"]
["지하1층 상부 보 석고보드 재설치","9.5t 방수보드 2ply","M2",20]
[]
["소   계"]
["9.도장공사"]
["1층 체육관 입구 좌우측 벽체 균열 보수","V-cutting","M",17]
["1층 체육관 입구 양측 벽체 도장","항곰팡이 페인트","M2",45]
["지하1층 상부 보 석고보드 도장","All putty, 항곰팡이 페인트","M2",20]
["지하1층 샤워실 벽체 도장 ","항곰팡이 페인트","M2",20]
[]
["소   계"]
["10.기타공사"]
["지하1층 누수 유도라인 공사","비닐, 유도 호스, 본공사 후 철거","식",1]
["남자샤워실 드레인 하부 유도배관 보강","하부 드레인 커버 배관 물넘침 보수","개소",1]
["지하1층 천장상부 슬래브 균열 보수",null,"M",10]
["지하1층 교수샤워실 락커 이동","1층 샤워실 본공사 전, 후","식",1]
["지하1층 교수샤워실 임시 칸막이 설치","샌드위치판넬 50mm","M2",7]
[]
["소   계"]